<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='NCP1400_5V_Step-Up_v11'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description: &lt;/span&gt;The NCP1400 is a 3.3V DC-DC converter. The breakout board will accept voltage inputs between 1 and 3 Volts (such as 1 or 2 AA batteries) and output a constant, low ripple 3.3V output capable of sourcing up to 100 mA. This board is great for supplying power to 3.3V sensors or providing 3.3V from a a single AA battery.&lt;br /&gt;


	&lt;br /&gt;


	The breakout board includes the necessary peripheral components. The input, ouput and ground pins are broken out on a 0.1&amp;quot; grid to allow easy access on a breadboard.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Prototyping/Batteries/NCP1400_33V_Step-Up_v11.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Prototyping/Batteries/Voltage_Switcher-NCP1400A-D.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>NCP1400 Step-Up Breakout</title>
<url>http://www.sparkfun.com/products/9216</url>
<tags>
<tag>Power</tag>
<tag>Step-Up</tag>
<tag>5V</tag>
<tag>3.3v</tag>
</tags>
<properties>
<property name='Input Voltage'>1-5V</property>
<property name='family'>Power Conditioning</property>
<property name='Output Voltage'>5V</property>
<property name='Connector'>0.1 Header</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/NCP1400_5V_Step-Up_v11_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/NCP1400_5V_Step-Up_v11_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/NCP1400_5V_Step-Up_v11_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/NCP1400_5V_Step-Up_v11_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector11' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='VOUT'>
<description>VOUT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
