<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='XBee-Regulated-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; The XBee Explorer Regulated takes care of the 3.3V regulation, signal conditioning, and basic activity indicators (Power, RSSI and DIN/DOUT activity LEDs). It translates the 5V signals to 3.3V so that you can connect a 5V (down to 3.3V) system to any XBee module. The board was conveniently designed to mate directly with Arduino Pro boards for &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=122&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;wireless bootloading&lt;/a&gt; and USB based configuration.&lt;br /&gt;


	&lt;br /&gt;


	This unit works with all XBee modules including the Series 1 and Series 2.5, standard and Pro versions. Plug an XBee into this breakout and you will have direct access to the serial and programming pins on the XBee unit and will be able to power the XBee with 5V.&lt;br /&gt;


	&lt;br /&gt;


	This board comes fully populated with 3.3V regulator (16V max input), XBee socket, four status LEDs, and a diode to allow 5V systems to communicate safely with the 3.3V XBees. This board does not include and XBee module. XBee modules sold below.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Regulated-v10.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;br /&gt;


		&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Regulated-v12.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.digi.com/support/kbase/kbaseresultdetl.jsp?kb=125&quot; target=&quot;_blank&quot;&gt;X-CTU Software&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorials/257&quot; target=&quot;_blank&quot;&gt;XBee Introduction and Buying Guide&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>XBee Explorer Regulated</title>
<url>http://www.sparkfun.com/products/9132</url>
<tags>
<tag>Xbee</tag>
<tag>Wireless</tag>
<tag>USB</tag>
<tag>Explorer</tag>
</tags>
<properties>
<property name='family'>Wireless</property>
<property name='Protocol'>XBee</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/XBee-Regulated-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/XBee-Regulated-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/XBee-Regulated-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/XBee-Regulated-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector8' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='DTR'>
<description>DTR</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='RES1'>
<description>RES1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='DIO11'>
<description>DIO11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='RSSI'>
<description>RSSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='male' name='DIO12'>
<description>DIO12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='DIN'>
<description>DIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='male' name='DOUT'>
<description>DOUT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='male' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
<connector id='connector18' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
</connector>
<connector id='connector19' type='male' name='DIO0'>
<description>DIO0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
</connector>
<connector id='connector20' type='male' name='DIO1'>
<description>DIO1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
</connector>
<connector id='connector21' type='male' name='DIO2'>
<description>DIO2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
</connector>
<connector id='connector22' type='male' name='DIO3'>
<description>DIO3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='RTS'>
<description>RTS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='male' name='DIO5'>
<description>DIO5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector25' type='male' name='RES2'>
<description>RES2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='male' name='DIO9'>
<description>DIO9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='male' name='CTS'>
<description>CTS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='male' name='DIO4'>
<description>DIO4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='male' name='DIO3'>
<description>DIO3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='male' name='DIN'>
<description>DIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='male' name='DOUT'>
<description>DOUT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector8'/>
<nodeMember connectorId='connector18'/>
<nodeMember connectorId='connector34'/>
<nodeMember connectorId='connector35'/>
</bus>
<bus id='dio3'>
<nodeMember connectorId='connector22'/>
<nodeMember connectorId='connector30'/>
</bus>
<bus id='din'>
<nodeMember connectorId='connector15'/>
<nodeMember connectorId='connector31'/>
</bus>
<bus id='dout'>
<nodeMember connectorId='connector16'/>
<nodeMember connectorId='connector32'/>
</bus>
<bus id='5v'>
<nodeMember connectorId='connector29'/>
<nodeMember connectorId='connector33'/>
</bus>
</buses>
</module>
