<?xml version='1.0' encoding='UTF-8'?>
<module referenceFile="Arduino_Leonardo_Rev3(fix).fzp" fritzingVersion="0.5.2b.02.18.4756" moduleId="EspruinoPico_8fb644a5b6642112445ed6d90bc494d8_6">
 <version replacedby="EspruinoPico">5</version>
 <date>Mon Nov 23 2015</date>
 <author>Gordon Williams</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Sans Serif'; font-size:9pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Verdana,Trebuchet MS,Arial,sans-serif'; font-size:8pt; color:#666666; background-color:#ffffff;">Espruino is an Interactive JavaScript interpreter for Microcontrollers, so you can program them quickly and easily. The Espruino Pico is a specially designed board with Espruino software pre-installed. It complements the Espruino software with masses of functionality and great battery life.&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <title>Espruino Pico</title>
 <url>http://www.espruino.com/Pico</url>
 <tags/>
 <properties>
  <property name="family">//obsolete//Espruino</property>
  <property name="variant">variant 1</property>
  <property name="part number"></property>
  <property name="layer"></property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/EspruinoPico_8fb644a5b6642112445ed6d90bc494d8_8_breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/EspruinoPico_8fb644a5b6642112445ed6d90bc494d8_8_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/EspruinoPico_8fb644a5b6642112445ed6d90bc494d8_8_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/EspruinoPico_8fb644a5b6642112445ed6d90bc494d8_8_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="female" name="Vin" id="connector6">
   <description>Battery Voltage In</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector6terminal" svgId="connector6pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector6pin"/>
     <p layer="copper1" svgId="connector6pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B15" id="connector7">
   <description>B15</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector7terminal" svgId="connector7pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector7pin"/>
     <p layer="copper1" svgId="connector7pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B14" id="connector8">
   <description>B14</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector8terminal" svgId="connector8pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector8pin"/>
     <p layer="copper1" svgId="connector8pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B13" id="connector9">
   <description>B13</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector9terminal" svgId="connector9pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector9pin"/>
     <p layer="copper1" svgId="connector9pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B10" id="connector11">
   <description>B10</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector11terminal" svgId="connector11pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector11pin"/>
     <p layer="copper1" svgId="connector11pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B1" id="connector12">
   <description>B1</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector12terminal" svgId="connector12pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector12pin"/>
     <p layer="copper1" svgId="connector12pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A7" id="connector13">
   <description>A7</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector13terminal" svgId="connector13pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector13pin"/>
     <p layer="copper1" svgId="connector13pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A6" id="connector14">
   <description>A6</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector14terminal" svgId="connector14pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector14pin"/>
     <p layer="copper1" svgId="connector14pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A5" id="connector15">
   <description>A5</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector15terminal" svgId="connector15pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector15pin"/>
     <p layer="copper1" svgId="connector15pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A4" id="connector16">
   <description>A4</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector16terminal" svgId="connector16pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector16pin"/>
     <p layer="copper1" svgId="connector16pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A3" id="connector17">
   <description>A3</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector17terminal" svgId="connector17pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector17pin"/>
     <p layer="copper1" svgId="connector17pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A2" id="connector18">
   <description>A2</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector18terminal" svgId="connector18pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector18pin"/>
     <p layer="copper1" svgId="connector18pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A1" id="connector19">
   <description>A1</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector19terminal" svgId="connector19pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector19pin"/>
     <p layer="copper1" svgId="connector19pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A0" id="connector20">
   <description>A0</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector20terminal" svgId="connector20pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector20pin"/>
     <p layer="copper1" svgId="connector20pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A10" id="connector21">
   <description>A10</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector21terminal" svgId="connector21pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector21pin"/>
     <p layer="copper1" svgId="connector21pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="A8" id="connector22">
   <description>A8</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector22terminal" svgId="connector22pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector22pin"/>
     <p layer="copper1" svgId="connector22pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B7" id="connector23">
   <description>B7</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector23terminal" svgId="connector23pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector23pin"/>
     <p layer="copper1" svgId="connector23pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B6" id="connector24">
   <description>B6</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector24terminal" svgId="connector24pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector24pin"/>
     <p layer="copper1" svgId="connector24pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B5" id="connector25">
   <description>B5</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector25terminal" svgId="connector25pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector25pin"/>
     <p layer="copper1" svgId="connector25pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B4" id="connector26">
   <description>B4</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector26terminal" svgId="connector26pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector26pin"/>
     <p layer="copper1" svgId="connector26pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B3" id="connector27">
   <description>B3</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector27terminal" svgId="connector27pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector27pin"/>
     <p layer="copper1" svgId="connector27pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="3.3" id="connector28">
   <description>3.3v Out</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector28terminal" svgId="connector28pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector28pin"/>
     <p layer="copper1" svgId="connector28pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="Vout" id="connector29">
   <description>Battery/USB Voltage Out</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector29terminal" svgId="connector29pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector29pin"/>
     <p layer="copper1" svgId="connector29pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="GND" id="connector40">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector40terminal" svgId="connector40pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector40pin"/>
     <p layer="copper1" svgId="connector40pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B9" id="connector41">
   <description>B9</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector41terminal" svgId="connector41pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector41pin"/>
     <p layer="copper1" svgId="connector41pin"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" name="B8" id="connector42">
   <description>B8</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector42terminal" svgId="connector42pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector42pin"/>
     <p layer="copper1" svgId="connector42pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
 </buses>
</module>
