<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Electromechanical-BATTERY-2-AA">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Electromechanical' BATTERY-2 AA -->
<version replacedby="Electromechanical-BATTERY-2-AA">4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>AA and AAA battery holders</description>
<title>BATTERY-2</title>
<tags>
<tag>AA</tag>
<tag>BATTERY-2</tag>
<tag>BATTERY-AA</tag>
</tags>
<properties>
<property name="package">battery-aa</property>
<property name="family">//obsolete//sparkfun Battery Holder</property>
<property name="variant">aa</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-electromechanical_battery-aa_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-electromechanical_battery-2_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-electromechanical_battery-aa_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-electromechanical_battery-aa_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector1" name="+1" type="male">
<description>+1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pad"/>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="+2" type="male">
<description>+2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="-1" type="male">
<description>-1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pad"/>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="-2" type="male">
<description>-2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>