<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b" moduleId="RFM12b_hope">
<version replacedby="RFM12b_hope_fix">3</version>
    <author>fabian althaus</author>
    <title>RFM12b HopeRF Transceiver</title>
    <label>RFM12b</label>
    <date>2014-06-11</date>
    <tags/>
    <properties>
        <property name="family">//obsolete//RFM12B Transreceiver</property>
        <property name="part number"/>
    </properties>
    <description>RF Transceiver by Hope RF.  Well supported Arduino libraries are available.  Part is available in several frequencies (433MHz, 915MHz)...</description>
    <views>
        <iconView>
            <layers image="icon/RFM12b_HopeRF_Transceiver__9c603c735b502.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/RFM12b_HopeRF_Transceiver.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/RFM12b_HopeRF_Transceiver__9c603c735b502.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/RFM12b_HopeRF_Transceiver__9c603c735b502.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper0"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="pad" id="connector3" name="4 DCLK/CFIL">
            <description>Clock output (no FIFO) / external filter cap</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector4" name="5 CLK">
            <description>Clock output for external microcontroller</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector5" name="6 nRES">
            <description>Reset output (active low)</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector6" name="7 GND">
            <description>Power ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector7" name="8 ANT">
            <description>Antenna</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector8" name="9 VDD">
            <description>Positive power supply</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector9" name="10 GND">
            <description>Power ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector10" name="11 nINT/VDI">
            <description>Interrupt input (active low) / Valid data indicator</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10erminal" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector11" name="12 SDI">
            <description>SPI data input</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                <p svgId="connector11pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector12" name="13 SCK">
            <description>SPI clock input</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector0" name="1 SDO">
            <description>Serial data output with bus hold</description>
            <views>
                <breadboardView>
                    <p svgId="connector0" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector13" name="14 nSEL">
            <description>Chip select (active low)</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector1" name="2 nIRQ">
            <description>Interrupts request output (active low)</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="pad" id="connector2" name="3 FSK/DATA">
            <description>Transmit FSK data input / Received data output</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
