<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.1223" moduleId="f80c6938-71e1-44a1-867e-442332a78ca8CapacitorModuleID">
 <version>4</version>
 <author>Mr.T</author>
 <title>Electrolytic Capacitor</title>
 <label>C</label>
 <date>2010-10-06</date>
 <tags>
  <tag>Electrolytic</tag>
  <tag>Capacitor</tag>
  <tag>fritzing core</tag>
 <tag>SMD</tag></tags>
 <properties>
  <property name="family">Capacitor [unidirectional]</property>
  <property name="capacitance" showInLabel="yes">10μF</property>
  <property name="package">0605 [SMD, electrolytic]</property>
    <property name="voltage" showInLabel="yes"/>
 </properties>
 <taxonomy>discreteParts.capacitor.elecrtolytic</taxonomy>
 <description>A smd electrolytic capacitor.</description>
 <views>
  <iconView>
   <layers image="icon/electrolytic_capacitor_small_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView fliphorizontal="true" flipvertical="true">
   <layers image="breadboard/electrolytic_capacitor_small_leg.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/capacitor_polar.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/SMD_elko_0605.svg">
     <layer layerId="silkscreen"/>
  <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="-" type="male">
   <description>- side</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"  legId="connector0leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="+" type="male">
   <description>+ side</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>