<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.1223" moduleId="1001ABDC03E">
 <version replacedby="MediumElectrolyticCapacitorModuleID">4</version>
 <author>Brendan Howell</author>
 <title>Electrolytic Capacitor</title>
 <label>C</label>
 <date>2008-12-22</date>
 <tags>
  <tag>Electrolytic</tag>
  <tag>Capacitor</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">//obsolete//Capacitor</property>
  <property name="Capacitance">470&#181;F</property>
  <property name="Capacitor Type">Electrolytic</property>
  <property name="Rated Voltage">35V</property>
 <property name="package">THT</property></properties>
 <taxonomy>discreteParts.capacitor.elecrtolytic</taxonomy>
 <description>470&#181;F electrolytic capacitor</description>
 <views>
  <iconView>
   <layers image="icon/electrolytic_capacitor_470uF_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView fliphorizontal="true" flipvertical="true">
   <layers image="breadboard/electrolytic_capacitor_470uF_35v.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/capacitor_polar.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/radial_can_200mil.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="-" type="male">
   <description>- side</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="+" type="male">
   <description>+ side</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>