<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.7.0b.02.01.5801" moduleId="17e42b0f30876b6ca457314cbd7e5847">
    <author>wreutz</author>
    <title>Color Sensor Breakout ADJD-S311</title>
    <url>http://www.sparkfun.com/products/10701</url>
    <date>2012-02-21</date>
    <tags>
        <tag>color</tag>
        <tag>sensor</tag>
        <tag>breakout</tag>
    </tags>
    <properties>
        <property name="family">Color Breakout</property>
        <property name="part number"/>
    </properties>
    <description>&lt;p>&lt;b>Description:&lt;/b>&lt;/p>
      &lt;p>The ADJD-S311-CR999 is a great little color light sensor. In fact, it's so little that it can be pretty difficult to play with, so we made this evaluation board! It provides all the necessary support circuitry to discern the smallest differences between visible colors.&lt;/p>

      &lt;p>&lt;b>Dimensions:&lt;/b> 21.6x12.7mm (0.85x0.50")&lt;/p>

      &lt;p>&lt;b>Documents:&lt;/b>&lt;/p>
      &lt;ul>
        &lt;li>
          &lt;a classname="" href="http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/LightImaging/ADJD-S311_Breakout-v10.pdf" name="" target="_blank">Schematic&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/LightImaging/ADJD-S311_Breakout-v10.zip" name="" target="_blank">Eagle Files&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/LightImaging/datasheetCR999.pdf" name="" target="_blank">Datasheet (ADJD-S311)&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://www.sparkfun.com/datasheets/Sensors/Imaging/adjd_s311_cr99_example.pde" name="" target="_blank">Example Arduino Code&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://www.sparkfun.com/datasheets/Sensors/Imaging/ADJD-S371-v11.zip" name="" target="_blank">Example PIC code&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://www.sparkfun.com/datasheets/Sensors/Imaging/ADJD-S371-v10-ARM.zip" name="" target="_blank">Example ARM code&lt;/a>
        &lt;/li>
        &lt;li>
          &lt;a classname="" href="http://bildr.org/2012/01/adjd-s311_arduino/" name="" target="_blank">Bildr Tutorial&lt;/a>
        &lt;/li>
</description>
    <views>
        <schematicView>
            <layers image="schematic/Color_Sensor_Breakout_ADJD_S311_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <iconView>
            <layers image="icon/Color_Sensor_Breakout_ADJD_S311_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <pcbView>
            <layers image="pcb/Color_Sensor_Breakout_ADJD_S311_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <breadboardView>
            <layers image="breadboard/Color_Sensor_Breakout_ADJD_S311_breadboard.svg">
                <layer layerId="breadboard"/>
                <layer layerId="icon"/>
            </layers>
        </breadboardView>
    </views>
    <connectors>
        <connector type="male" id="connector3" name="SCL">
            <description>SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector3" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3" layer="copper1"/>
                    <p svgId="connector3" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="SDA">
            <description>SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector4" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4" layer="copper1"/>
                    <p svgId="connector4" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="CLK">
            <description>Clock</description>
            <views>
                <breadboardView>
                    <p svgId="connector5" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5" layer="copper1"/>
                    <p svgId="connector5" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="SLP">
            <description>SLEEP</description>
            <views>
                <breadboardView>
                    <p svgId="connector6" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6" layer="copper1"/>
                    <p svgId="connector6" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector7" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7" layer="copper1"/>
                    <p svgId="connector7" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector0" name="LED">
            <description>LED enable/disable</description>
            <views>
                <breadboardView>
                    <p svgId="connector0" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0" layer="copper1"/>
                    <p svgId="connector0" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="VCC">
            <description>3.3V</description>
            <views>
                <breadboardView>
                    <p svgId="connector1" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1" layer="copper1"/>
                    <p svgId="connector1" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector2" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2" layer="copper1"/>
                    <p svgId="connector2" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
