<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.5b.07.02.6130" moduleId="92173317483b1d9a9a78868e2704aeeb">
    <version replacedby="DS18B20">1</version>
    <author>John De Cristofaro for Adafruit Industries</author>
    <title>DS18B20 1-Wire Temperature Sensor</title>
    <label>DS</label>
    <date>2012-08-07</date>
    <url>http://www.maxim-ic.com/datasheet/index.mvp/id/2812</url>
    <tags>
        <tag>temp</tag>
        <tag>thermometer</tag>
        <tag>maxim</tag>
        <tag>sensor</tag>
    </tags>
    <properties>
        <property name="family">//obsolete//sensor</property>
        <property name="part number">DS18B20</property>
    </properties>
    <description>DS18B20 1-Wire Temperature Sensor</description>
    <views>
        <iconView>
            <layers image="icon/DS18B20__5240d891e23cace35a4de6acc361c04__icon__d53cbcd19f32fb9a9236373b10833a61.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/DS18B20__5240d891e23cace35a4de6acc361c04__breadboard__7b535917175078873c2dd8e438e15652.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/DS18B20__5240d891e23cace35a4de6acc361c04__schematic__7051cf864e168372439496e5f0a88453.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/DS18B20__5240d891e23cace35a4de6acc361c04__pcb__1d5382571b4af4033f2c8ff3b34d64f3.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" type="male" name="VDD">
            <description>Supply voltage (3-5V)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper1" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="GND">
            <description>ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="DQ">
            <description>1-Wire Data</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper1" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
