<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.11" moduleId="415c9d899a1e7de6c023ea0731bab117"><version>4</version>
    <author>Lionel Michel</author>
    <title>Microphone</title>
    <label>MIC</label>
    <date>2009-11-12</date>
    <tags>
     <tag>microphone</tag>
    <tag>input</tag>
     <tag>audio</tag>
      <tag>sensor</tag>
      </tags>
    <properties>
        <property name="family">Microphone</property>
    </properties>
    <views>
        <iconView>
            <layers image="icon/microphone.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/microphone.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/microphone.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper_2_100mil_pcb.svg">
                <layer layerId="copper0"/>
		<layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="pin1" type="male">
            <description>Pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin2" type="male">
            <description>Pin 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>