<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.4.4" moduleId="7.5mmPPCapacitor_CapacitorModuleID">
    <version>4</version>
    <author>Fritzing Team</author>
    <title>Film/Foil Capacitor</title>
    <label>C</label>
    <date>2017-01-15</date>
    <tags>
        <tag>film/foil</tag>
        <tag>polypropylene</tag>
        <tag>capacitor pp</tag>
        <tag>pp</tag>
        <tag>capacitor</tag>
        <tag>fritzing core</tag>
    </tags>
  <properties>
  	<property name="family">Capacitor [pp]</property>
  	<property name="Capacitance7.5mm" showInLabel="yes">1&#x3BC;F</property>
    <property name="package">7.5mm [THT, pp]</property>
   <property name="voltageHigh" showInLabel="yes"></property>
 </properties>
    <description>Polypropylene/Film and Foil capacitor.</description>
 <spice><line>C{instanceTitle} {net connector0} {net connector1} {capacitance} IC=0</line></spice>
    <views>
        <iconView>
            <layers image="icon/capacitor_pp.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView  fliphorizontal="true" flipvertical="true">
            <layers image="breadboard/capacitor_pp_7.5mm_leg.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/capacitor_pp.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/capacitor_pp_7.5mm_pcb.svg">
                <layer layerId="copper0"/>
	      <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="-" type="male">
            <description>negative side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="+" type="male">
            <description>positive side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>
