<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="JST-B3P-VH" referenceFile="generic_male_pin_header_3_0.156in.fzp" fritzingVersion="0.2.2.b.03.04.2550">
 <version>4</version>
 <author>Stephen G. Parry</author>
 <title>JST-B3P-VH</title>
 <label>J</label>
 <date>Thu Jun 16 2016</date>
 <tags/>
 <properties>
  <property name="family">JST VH Pin Header</property>
  <property name="variant">- Male 3 pin header</property>
  <property name="hole size"></property>
  <property name="part number">JST-B3P-VH</property>
  <property name="Pin Spacing">0.156in (3.96mm)</property>
  <property name="Form">♂ (male)</property>
  <property name="Pins">3</property>
  <property name="layer"></property>
  <property name="Position"></property>
  <property name="Row">single</property>
  <property name="package">THT</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">JST-B3P-VH&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">Male 3 pin header from JST VH series.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">The female partner connector (JST-VHR-3N) to this is used on Dagu motors in their robots. This part is not breadboard or stripboard friendly - the pin spacings are not properly compatible. However, you can make the part fit by drilling between the tracks for the outer connectors and soldering a trace across them. This can be represented in Frtizing using additional wires. This has the secondary benefit of increasing current carrying capacity.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:'Oxygen-Sans'; font-size:10pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">When plugging the female connector onto this, ensure that the correct connectors on the female have located.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:'Oxygen-Sans'; font-size:10pt;">&lt;br />&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/JST-B3P-VH_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/JST-B3P-VH_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true">
   <layers image="schematic/JST-B3P-VH_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/JST-B3P-VH_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector name="pin2" id="connector0" type="male">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="pin1" id="connector1" type="male">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="pin3" id="connector2" type="male">
   <description>pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
