<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.2b.08.04.4392" moduleId="0b6deb11c8005423ea8d84452203654d">
    <author>tigoe</author>
    <title>HCMS-29xx</title>
    <label>HCMS-29XX</label>
    <date>2010-03-11</date>
    <tags>
        <tag>LED Display</tag>
    </tags>
    <properties>
        <property name="family">LED Display</property>
    </properties>
    <description>HCMS-29XX LED display from Avago</description>
    <views>
        <iconView>
            <layers image="icon/HCMS-29xxff.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/HCMS-29xxff.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/HCMS-29xxff.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/HCMS-29xxff.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="male" id="connector3" name="VLED">
            <description>no description yet</description>
            <views>
                <breadboardView>
                    <p svgId="connector3" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3" layer="copper1"/>
                    <p svgId="connector3" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="Data In">
            <description>Data Input Pin</description>
            <views>
                <breadboardView>
                    <p svgId="connector4" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4" layer="copper1"/>
                    <p svgId="connector4" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="RS">
            <description>Register Select</description>
            <views>
                <breadboardView>
                    <p svgId="connector5" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5" layer="copper1"/>
                    <p svgId="connector5" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="Clock">
            <description>Data Clock input</description>
            <views>
                <breadboardView>
                    <p svgId="connector6" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6" layer="copper1"/>
                    <p svgId="connector6" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="Chip Enable">
            <description>Chip Enable Pin</description>
            <views>
                <breadboardView>
                    <p svgId="connector7" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7" layer="copper1"/>
                    <p svgId="connector7" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector8" name="Blank">
            <description>Blanking Pin</description>
            <views>
                <breadboardView>
                    <p svgId="connector8" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8" layer="copper1"/>
                    <p svgId="connector8" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="GND Logic">
            <description>Ground for logic in the IC</description>
            <views>
                <breadboardView>
                    <p svgId="connector9" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9" layer="copper1"/>
                    <p svgId="connector9" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="SEL">
            <description>Select internal or external oscillator</description>
            <views>
                <breadboardView>
                    <p svgId="connector10" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10" layer="copper1"/>
                    <p svgId="connector10" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="V Logic">
            <description>Voltage supply for onboard logic</description>
            <views>
                <breadboardView>
                    <p svgId="connector11" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11" layer="copper1"/>
                    <p svgId="connector11" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="Reset">
            <description>Reset pin</description>
            <views>
                <breadboardView>
                    <p svgId="connector12" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12" layer="copper1"/>
                    <p svgId="connector12" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="V LED">
            <description>Voltage supply for LEDs</description>
            <views>
                <breadboardView>
                    <p svgId="connector1" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1" layer="copper1"/>
                    <p svgId="connector1" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="Osc.">
            <description>Input for external oscillator</description>
            <views>
                <breadboardView>
                    <p svgId="connector13" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13" layer="copper1"/>
                    <p svgId="connector13" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="Data Out">
            <description>Data output</description>
            <views>
                <breadboardView>
                    <p svgId="connector14" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14" layer="copper1"/>
                    <p svgId="connector14" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="Gnd LED">
            <description>Ground for the LEDs</description>
            <views>
                <breadboardView>
                    <p svgId="connector2" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2" layer="copper1"/>
                    <p svgId="connector2" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
