<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.0.b.02.26.2493" moduleId="56bed03878064b8286b71d5240035138">
<version replacedby="56bed03878064b8286b71d5240035138InductorModuleID">4</version>
    <author>lionel</author>
    <title>Inductor</title>
    <label>L</label>
    <date>2009-02-26</date>
    <tags>
        <tag>inductor</tag>
        <tag>coil</tag>
    </tags>
    <properties>
        <property name="family">//obsolete//air-core inductor</property>
    <property name="package">400 mil [THT]</property>
     <property name="inductance" showInLabel="yes">10nH</property>
     </properties>
    <description>Inductor</description>
    <views>
        <iconView>
            <layers image="icon/inductor.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/inductor.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
         <schematicView fliphorizontal="true" flipvertical="true">
            <layers image="schematic/inductor.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/inductor_400mil.svg">
              <layer layerId="copper0"/>
              <layer layerId="copper1"/>
              <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="pin 0" type="male">
            <description>pin 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin 1" type="male">
            <description>pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                    <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
