<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="RFM23BP_83dca743edce69d8624555bae587be66_7" referenceFile="BMP085 Breakout-v13.fzp">
 <version replacedby="RFM23BP">4</version>
 <date>sam. mars 26 2016</date>
 <author>le hoop</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Ubuntu'; font-size:11pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:12px; margin-bottom:12px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8pt; font-weight:600;">Description: &lt;/span>&lt;span style=" font-family:'sans-serif'; font-size:15px;">HopeRF's RFM23BP are highly integrated, low cost,433/868/915MHZ &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">wireless ISM transceivers module. &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">The low receive sensitivity&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif';">(–120dBm) &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">coupled with industry leading +30dBm output power ensures &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif';">extended &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">range and &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">improved link performance. Built-in antenna diversity and &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">support for frequency hopping can be us&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">ed to further extend range and enhance &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">performance. &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">Additional system features such as &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">an automatic &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">wake-up &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">timer, low &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">battery detector, 64 byte TX/RX FIFOs, &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">automatic packet handling, and preamble &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">detection reduce overall current consum&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">ption and allow the use of lower-cost &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">system MCUs. An integrated temperatur&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">e sensor, general purpose ADC, power- &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">on-reset (POR), and GPIOs further reduce overall system cost and size. &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">The RFM23BP digital receive archit ec&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">ture features a high-performance ADC &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">and DSP based modem which performs dem&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">odulation, filtering, and packet &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">handling for increased flexibility and performance. The direct digital transmit &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">modulation and automatic PA power rampin&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">g ensure precise transmit modulation &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">and reduced spectral spreading ensuring compliance with global regulations &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">including FCC, ETSI. &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">An easy-to-use calculator is provided &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">to quickly configure the radio settings, &lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'sans-serif'; font-size:15px;">simplifying customer's system design and reducing time to market.&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <title>RFM23BP</title>
 <url>www.lehoop.fr</url>
 <tags>
  <tag>433mhz</tag>
  <tag>rfm23bp</tag>
  <tag>ism</tag>
 </tags>
 <properties>
  <property name="family">//obsolete//lehoop</property>
  <property name="variant">variant 1</property>
  <property name="layer"></property>
  <property name="part number"></property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/RFM23BP_28f0aeb1c8ab1c048f7c7ebd3fa05abe_1_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/RFM23BP_28f0aeb1c8ab1c048f7c7ebd3fa05abe_1_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/RFM23BP_28f0aeb1c8ab1c048f7c7ebd3fa05abe_1_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/RFM23BP_28f0aeb1c8ab1c048f7c7ebd3fa05abe_1_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="male" id="connector5" name="ANT">
   <description>ANT</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pad" layer="copper0"/>
     <p svgId="connector5pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector6" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pad" layer="copper0"/>
     <p svgId="connector6pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="SDO">
   <description>SDO</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pad" layer="copper0"/>
     <p svgId="connector7pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector8" name="SDI">
   <description>SDI</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pad" layer="copper0"/>
     <p svgId="connector8pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="SCK">
   <description>SCK</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pad" layer="copper0"/>
     <p svgId="connector9pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector10" name="NSEL">
   <description>NSEL</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pad" layer="copper0"/>
     <p svgId="connector10pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector11" name="NIRQ">
   <description>NIRQ</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector12" name="SDN">
   <description>SDN</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector14" name="GPIO_2">
   <description>GPIO_2</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector15" name="GPIO_1">
   <description>GPIO_1</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard" terminalId="connector15terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector16" name="GPIO_0">
   <description>GPIO_0</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard" terminalId="connector16terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector17" name="VCC">
   <description>VCC</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector18" name="RXON">
   <description>RXON</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector19" name="TXON">
   <description>TXON</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector20" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector21" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="internal1"/>
  <bus id="internal2">
   <nodeMember connectorId="connector21"/>
   <nodeMember connectorId="connector6"/>
   <nodeMember connectorId="connector20"/>
  </bus>
 </buses>
</module>
