<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="ESP8266_7_723ce4de09d714597656302fbbc6971c_17" referenceFile="Barometric Pressure Sensor.fzp">
  <version replacedby="ESP8266_7">1</version>
 <author>YDonnelly; Geert Roumen; greg-ware; Simone Picchioni + fix:f.althaus</author>
 <title>ESP8266 WiFi Module</title>
 <label>U</label>
 <date>Tue Jul 28 2015</date>
 <tags>
  <tag>breakout</tag>
  <tag>radio</tag>
  <tag>ESP8266</tag>
  <tag>wifi</tag>
  <tag>module</tag>
 </tags>
 <properties>
  <property name="variant">variant 7</property>
  <property name="family">//obsolete//ESP8266</property>
  <property name="part number">ESP8266</property>
  <property name="layer"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Ubuntu'; font-size:11pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">Generic WiFi Module based on the ESP8266 with onboard PCB antenna and UART communications&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/ESP8266_7_3d9a9742b08b59b877d1a9c22c0ed5dc_3_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/ESP8266_7_3d9a9742b08b59b877d1a9c22c0ed5dc_3_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <breadboardView>
   <layers image="breadboard/ESP8266_7_3d9a9742b08b59b877d1a9c22c0ed5dc_3_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <pcbView>
   <layers image="pcb/ESP8266_7_3d9a9742b08b59b877d1a9c22c0ed5dc_3_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="pad" id="connector4" name="GPIO_2">
   <description>General-Purpose IO 2</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector5" name="CH_PD">
   <description>Enable (Active High)</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector6" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector0" name="RXD">
   <description>UART Receive</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector1" name="VCC">
   <description>+3.3V Supply</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector2" name="GPIO_0">
   <description>General-Purpose IO 0</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector7" name="TXD">
   <description>UART Transmit</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector8" name="GPIO_15">
   <description>General-Purpose IO 15</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector9" name="GPIO_4">
   <description>General-Purpose IO 4</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector10" name="GPIO_5">
   <description>General-Purpose IO 5</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector11" name="ADC_0">
   <description>Analog-Digital-Converter</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector12" name="GPIO_16">
   <description>General-Purpose IO 16</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector13" name="GPIO_14">
   <description>General-Purpose IO 14</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector14" name="GPIO_12">
   <description>General-Purpose IO 12</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector15" name="GPIO_13">
   <description>General-Purpose IO 13</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="pad" id="connector16" name="REST">
   <description>Reset</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>http://www.esp8266.com</url>
</module>
