<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.9.3b" moduleId="Gizwits_WiFi_Witty_ESP_12F">
 <version>1</version>
 <author>Mike Causer</author>
 <title>Gizwits WiFi Witty ESP-12F</title>
 <label>Gizwits WiFi Witty ESP-12F</label>
 <date>Sat Feb 13 2016</date>
 <url>http://site.gizwits.com/en/developer/</url>
 <tags>
  <tag>Microcontroller</tag>
  <tag>ESP8266</tag>
  <tag>ESP-12F</tag>
  <tag>WiFi</tag>
  <tag>LDR</tag>
  <tag>RGB-LED</tag>
  <tag>WS2812</tag>
  <tag>CH340</tag>
  <tag>Arduino</tag>
  <tag>NodeMCU</tag>
 </tags>
 <properties>
  <property name="family">Gizwits WiFi Witty ESP-12F</property>
  <property name="variant">variant 1</property>
  <property name="part number"></property>
  <property name="layer"></property>
 </properties>
 <description>A breadboard friendly two part WiFi development board by Gizwits, powered by an ESP8266 ESP-12F SoC, featuring twin micro-usb ports, a photoresistor, a WS2812 RGB-LED and three buttons. The board comes in two parts. The bottom half has reset and flash buttons, a micro-usb with CH340 UART and 2x 1x08 female headers. The top half has the ESP-12F, LDR, RGB-LED, micro-usb (for power only), an input button and 2x 1x08 male headers which fill an entire breadboard (12 pins wide).</description>
 <views>
  <iconView>
   <layers image="breadboard/Gizwits-WiFi-Witty-ESP-12F_breadboard.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/Gizwits-WiFi-Witty-ESP-12F_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/Gizwits-WiFi-Witty-ESP-12F_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Gizwits-WiFi-Witty-ESP-12F_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" type="male" name="REST">
   <description>Reset</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pad" layer="copper0"/>
     <p svgId="connector0pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" type="male" name="ADC">
   <description>ADC</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pad" layer="copper0"/>
     <p svgId="connector1pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="male" name="CH_PD">
   <description>CH_PD</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pad" layer="copper0"/>
     <p svgId="connector2pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="male" name="GPIO16">
   <description>GPIO16</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pad" layer="copper0"/>
     <p svgId="connector3pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="GPIO14">
   <description>GPIO14</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pad" layer="copper0"/>
     <p svgId="connector4pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="GPIO12">
   <description>GPIO12</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pad" layer="copper0"/>
     <p svgId="connector5pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="male" name="GPIO13">
   <description>GPIO13</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pad" layer="copper0"/>
     <p svgId="connector6pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="VCC">
   <description>VCC</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pad" layer="copper0"/>
     <p svgId="connector7pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="male" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" terminalId="connector8terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pad" layer="copper0"/>
     <p svgId="connector8pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="male" name="GPIO15">
   <description>GPIO15</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" terminalId="connector9terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pad" layer="copper0"/>
     <p svgId="connector9pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="male" name="GPIO2">
   <description>GPIO2</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" terminalId="connector10terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pad" layer="copper0"/>
     <p svgId="connector10pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="male" name="GPIO0">
   <description>GPIO0</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" terminalId="connector11terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pad" layer="copper0"/>
     <p svgId="connector11pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="male" name="GPIO4">
   <description>GPIO4</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" terminalId="connector12terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pad" layer="copper0"/>
     <p svgId="connector12pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="male" name="GPIO5">
   <description>GPIO5</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" terminalId="connector13terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pad" layer="copper0"/>
     <p svgId="connector13pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" type="male" name="RXD">
   <description>RXD</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" terminalId="connector14terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pad" layer="copper0"/>
     <p svgId="connector14pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="male" name="TXD">
   <description>TXD</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" terminalId="connector15terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pad" layer="copper0"/>
     <p svgId="connector15pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
