<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module fritzingVersion="0.1.1255" moduleId="1238DBdfgDC00-vofdghfhjaer">
  <version>5</version>
  <author>Mr.T</author>
  <title>Voltage Regulator - 5V</title>
  <label>U</label>
  <date>2018-4-24</date>
  <tags>
    <tag>regulator</tag>
    <tag>7805</tag>
    <tag>power</tag>
    <tag>fritzing core</tag>
    <tag>SMD</tag>
  </tags>
  <properties>
    <property name="package">DPak [SMD]</property>
    <property name="voltage">5V</property>
    <property name="family">Voltage Regulator</property>
  </properties>
  <description>5V DC Voltage Regulator</description>
  <views>
    <iconView>
      <layers image="icon/voltage_regulator_vreg_icon.svg">
        <layer layerId="icon"/>
      </layers>
    </iconView>
    <breadboardView>
      <layers image="breadboard/voltage_regulator_vreg.svg">
        <layer layerId="breadboard"/>
      </layers>
    </breadboardView>
    <schematicView>
      <layers image="schematic/voltage_regulator_5v.svg">
        <layer layerId="schematic"/>
      </layers>
    </schematicView>
    <pcbView>
      <layers image="pcb/SMD_DPak.svg">
        <layer layerId="silkscreen"/>
        <layer layerId="copper1"/>
      </layers>
    </pcbView>
  </views>
  <connectors>
    <connector id="connector0" name="input voltage" type="male">
      <description>input</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
        </breadboardView>
        <schematicView>
          <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper1" svgId="connector0pad"/>
        </pcbView>
      </views>
    </connector>
    <connector id="connector1" name="GND" type="male">
      <description>ground</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
        </breadboardView>
        <schematicView>
          <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper1" svgId="connector1pad"/>
        </pcbView>
      </views>
    </connector>
    <connector id="connector2" name="output voltage" type="male">
      <description>output voltage</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector2pin" legId="connector2leg"/>
        </breadboardView>
        <schematicView>
          <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper1" svgId="connector2pad"/>
        </pcbView>
      </views>
    </connector>
  </connectors>
</module>
