<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-DiscreteSemi-TRANSISTOR_NPN-SOT89">
<!-- generated from Sparkfun Eagle Library 'SparkFun-DiscreteSemi' TRANSISTOR_NPN SOT89 -->
<version>4</version>
<date>2013-02-13</date>
<label>Q</label>
<author>www.fritzing.org</author>
<description>Generic NPN BJT. MMBT2222 is the common NPN we use. Double check against datasheet- not all devices are the same!</description>
<title>TRANSISTOR_NPN</title>
<tags>
<tag>SOT89</tag>
<tag>TRANSISTOR_NPN</tag>
</tags>
<properties>
<property name="package">sot89</property>
<property name="family">sparkfun Transistor NPN</property>
<property name="variant">sot89</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-discretesemi_sot89_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-discretesemi_npn_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-discretesemi_sot89_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-discretesemi_sot89_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="B" type="male">
<description>B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="C" type="male">
<description>C</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="E" type="male">
<description>E</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>