<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b.04.10.5970" moduleId="96boards_CE_fixed" referenceFile="96boards_CE.fzp">
 <version>2</version>
 <author>Ricardo Salveti fixed by f.althaus</author>
 <title>96boards Consumer Edition</title>
 <label>96boards CE</label>
 <date>Mon May 16 2016</date>
 <url>http://www.96boards.org</url>
 <tags>
  <tag>96boards</tag>
  <tag>CE</tag>
 </tags>
 <properties>
  <property name="variant">96boards CE</property>
  <property name="family">cpu board (96boards)</property>
  <property name="layer"></property>
  <property name="part number"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Ubuntu'; font-size:11pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">96boards is the first open specification to define a platform for the delivery of compatible low-cost, small footprint 32-bit and 64-bit Cortex-A boards from the range of ARM SoC vendors. Standardized expansion buses for peripheral I/O, display and cameras allow the hardware ecosystem to develop a range of compatible add-on products that will work on any 96Boards product over the lifetime of the platform.&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">This part includes the low expansion headers for the Consumer Edition specification.&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/96boards_CE_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/96boards_CE_breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/96boards_CE_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/96boards_CE_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector1" type="female" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboardbreadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="female" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboardbreadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="female" name="UART0_CTS">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboardbreadboard" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="female" name="PWR_BTN_N">
   <description>Power Button</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboardbreadboard" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="female" name="UART0_TxD">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboardbreadboard" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="female" name="RST_BTN_N">
   <description>Reset Button</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboardbreadboard" terminalId="connector6terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="female" name="UART0_RxD">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboardbreadboard" terminalId="connector7terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="female" name="SPI0_SCLK">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboardbreadboard" terminalId="connector8terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="female" name="UART0_RTS">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboardbreadboard" terminalId="connector9terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="female" name="SPI0_DIN">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboardbreadboard" terminalId="connector10terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="female" name="UART1_TxD">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboardbreadboard" terminalId="connector11terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="female" name="SPI0_CS">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboardbreadboard" terminalId="connector12terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="female" name="UART1_RxD">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboardbreadboard" terminalId="connector13terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" type="female" name="SPI0_DOUT">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboardbreadboard" terminalId="connector14terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="female" name="I2C0_SCL">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboardbreadboard" terminalId="connector15terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector16" type="female" name="PCM_FS">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboardbreadboard" terminalId="connector16terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector17" type="female" name="I2C_SDA">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboardbreadboard" terminalId="connector17terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector18" type="female" name="PCM_CLK">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboardbreadboard" terminalId="connector18terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector19" type="female" name="I2C1_SCL">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboardbreadboard" terminalId="connector19terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector20" type="female" name="PCM_DO">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboardbreadboard" terminalId="connector20terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector21" type="female" name="I2C1_SDA">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboardbreadboard" terminalId="connector21terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector22" type="female" name="PCM_DI">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboardbreadboard" terminalId="connector22terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector23" type="female" name="GPIO-A">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboardbreadboard" terminalId="connector23terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector24" type="female" name="GPIO-B">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboardbreadboard" terminalId="connector24terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector25" type="female" name="GPIO-C">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboardbreadboard" terminalId="connector25terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector26" type="female" name="GPIO-D">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboardbreadboard" terminalId="connector26terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector27" type="female" name="GPIO-E">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboardbreadboard" terminalId="connector27terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector28" type="female" name="GPIO-F">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboardbreadboard" terminalId="connector28terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector29" type="female" name="GPIO-G">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboardbreadboard" terminalId="connector29terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector30" type="female" name="GPIO-H">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboardbreadboard" terminalId="connector30terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector31" type="female" name="GPIO-I">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboardbreadboard" terminalId="connector31terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector32" type="female" name="GPIO-J">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" layer="breadboardbreadboard" terminalId="connector32terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector33" type="female" name="GPIO-K">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector33pin" layer="breadboardbreadboard" terminalId="connector33terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector33pin" layer="copper0"/>
     <p svgId="connector33pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector34" type="female" name="GPIO-L">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector34pin" layer="breadboardbreadboard" terminalId="connector34terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector34pin" layer="copper0"/>
     <p svgId="connector34pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector35" type="female" name="1V8">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector35pin" layer="breadboardbreadboard" terminalId="connector35terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector35pin" layer="copper0"/>
     <p svgId="connector35pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector36" type="female" name="SYS_DCIN">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector36pin" layer="breadboardbreadboard" terminalId="connector36terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector36pin" layer="copper0"/>
     <p svgId="connector36pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector37" type="female" name="5V">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector37pin" layer="breadboardbreadboard" terminalId="connector37terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector37pin" layer="schematic" terminalId="connector37terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector37pin" layer="copper0"/>
     <p svgId="connector37pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector38" type="female" name="SYS_DCIN">
   <description></description>
   <views>
    <breadboardView>
     <p svgId="connector38pin" layer="breadboardbreadboard" terminalId="connector38terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector38pin" layer="schematic" terminalId="connector38terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector38pin" layer="copper0"/>
     <p svgId="connector38pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector39" type="female" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector39pin" layer="breadboardbreadboard" terminalId="connector39terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector39pin" layer="copper0"/>
     <p svgId="connector39pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector40" type="female" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector40pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector40pin" layer="copper0"/>
     <p svgId="connector40pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="GND">
   <nodeMember connectorId="connector39"/>
   <nodeMember connectorId="connector40"/>
   <nodeMember connectorId="connector1"/>
   <nodeMember connectorId="connector2"/>
  </bus>
  <bus id="DCIN">
   <nodeMember connectorId="connector38"/>
   <nodeMember connectorId="connector36"/>
  </bus>
 </buses>
</module>
