<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.3b.09.26.4458" moduleId="961807c738804558a7a2-403120c513dc">
    <version>4</version>
    <author>Petris Christian</author>
    <title>SN74LS20N</title>
    <label>U</label>
    <date>2011-02-22</date>
    <tags>
        <tag>DIP</tag>
        <tag>TTL</tag>
        <tag>Logic IC</tag>
        <tag>74xx</tag>
        <tag>Logic Gates</tag>
        <tag>NAND</tag>
    </tags>
    <properties>
        <property name="family">74xx Series</property>
        <property name="type">SN74LS20N</property>
        <property name="package">DIP14 [THT]</property>
    </properties>
    <description>Dual 4-Input Positive-NAND Gates</description>
    <views>
        <pcbView>
            <layers image="pcb/SN74LS20N_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="icon/SN74LS20N_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/SN74LS20N_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/SN74LS20N_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector type="male" id="connector3" name="1C">
            <description>in part 4</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper1"/>
                    <p svgId="connector3pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="1D">
            <description>in part 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper1"/>
                    <p svgId="connector4pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="1Y">
            <description>out NAND 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper1"/>
                    <p svgId="connector5pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="GND">
            <description>digital ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper1"/>
                    <p svgId="connector6pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="2Y">
            <description>out NAND 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper1"/>
                    <p svgId="connector7pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector8" name="2A">
            <description>in part 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper1"/>
                    <p svgId="connector8pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="2B">
            <description>in part 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper1"/>
                    <p svgId="connector9pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper1"/>
                    <p svgId="connector10pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="2C">
            <description>in part 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pin" layer="copper1"/>
                    <p svgId="connector11pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="2D">
            <description>in part 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper1"/>
                    <p svgId="connector12pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector0" name="1A">
            <description>in part 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper1"/>
                    <p svgId="connector0pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="1B">
            <description>in part 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper1"/>
                    <p svgId="connector1pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="VCC">
            <description>power simpply +5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper1"/>
                    <p svgId="connector13pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper1"/>
                    <p svgId="connector2pin" layer="copper0"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
