<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.3b" moduleId="rtc_ds3231_breakout">
 <version>7</version>
 <date>Sun Jul 26 2015</date>
 <label>ZS-042 RTC</label>
 <author>Richard Bruneau, f.althaus</author>
 <description>This is the ZS-042 RTC module which uses the Maxim DS3231 real time clock IC. The module has a battery holder for a LIR2032 or CR2032. The module also includes an Atmel AT24C32 32K EEPROM for storing important information. The module can operate at 3V3 and 5V.</description>
 <title>ZS-042 RTC Module</title>
 <tags>
  <tag>AT24C32</tag>
  <tag>ZS-042</tag>
  <tag>clock</tag>
  <tag>DS3231</tag>
  <tag>RTC</tag>
 </tags>
 <properties>
  <property name="chip">DS3231</property>
  <property name="family">rtc</property>
  <property name="variant">variant 4</property>
  <property name="layer"></property>
  <property name="part number"></property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/rtc_ds3231_breakout_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/rtc_ds3231_breakout_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/rtc_ds3231_breakout_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/rtc_ds3231_breakout_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="female" id="connector0" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pad" layer="copper1"/>
     <p svgId="connector0pad" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector1" name="VCC">
   <description>VCC</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pad" layer="copper1" terminalId="connector1terminal"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector2" name="SDA">
   <description>SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pad" layer="copper1"/>
     <p svgId="connector2pad" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector3" name="SCL">
   <description>SCL</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pad" layer="copper1"/>
     <p svgId="connector3pad" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector4" name="SQW">
   <description>SQW</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector5" name="32K">
   <description>32K</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper1"/>
     <p svgId="connector5pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector6" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper1"/>
     <p svgId="connector6pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector7" name="VCC">
   <description>VCC</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper1"/>
     <p svgId="connector7pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector8" name="SDA">
   <description>SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper1"/>
     <p svgId="connector8pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector9" name="SCL">
   <description>SCL</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper1"/>
     <p svgId="connector9pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses/>
 <url/>
</module>
