<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.7.2b.03.19.5922" moduleId="849f978c8022bc21e03c01a989238882" referenceFile="LM124-324_Quad_Opamp.fzp">
 <version>4</version>
 <author>Andre van Ooijen</author>
 <title>LM124-324 Quad Opamp</title>
 <label>U</label>
 <date>ma apr. 8 2013</date>
 <tags>
  <tag>user part</tag>
  <tag>DIP</tag>
 </tags>
 <properties>
  <property name="family">Quad Opamp</property>
  <property name="variant">variant 1</property>
  <property name="package">DIP (Dual Inline)</property>
  <property name="chip label">LM124-324</property>
  <property name="part number"></property>
  <property name="pins">14</property>
  <property name="spacing">300mil</property>
 </properties>
 <description>A Quadruple Operational Amplifier (Opamp)</description>
 <views>
  <breadboardView>
   <layers image="breadboard/svg.breadboard.LM124-324_Quad_Opamp.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/svg.schematic.LM124-324_Quad_Opamp.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/svg.pcb.LM124-324_Quad_Opamp.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/svg.icon.LM124-324_Quad_Opamp.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="1OUT">
   <description>Output 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="1IN-">
   <description>Inverting Input 1</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="1IN+">
   <description>Non-inverting Input 1</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="VCC+">
   <description>Positive Input Voltage (+3.5V to +18V)</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="2IN+">
   <description>Non-inverting Input 2</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector5" name="2IN-">
   <description>Inverting Input 2</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector6" name="2OUT">
   <description>Output 2</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="3OUT">
   <description>Output 3</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector8" name="3IN-">
   <description>Inverting Input 3</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="3IN+">
   <description>Non-inverting Input 3</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector10" name="VCC-">
   <description>Negative Input Voltage (-3.5V to -18V)</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector11" name="4IN+">
   <description>Non-inverting Input 4</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector12" name="4IN-">
   <description>Inverting Input 4</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector13" name="4OUT">
   <description>Output 4</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
