<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='audiojack_breakout-v11'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Replacement:&lt;/strong&gt; &lt;a href=&quot;http://www.sparkfun.com/products/10588&quot; target=&quot;_blank&quot;&gt;PRT-10588&lt;/a&gt;. The new revision corrects the silkscreen so that the pins are now labeled correctly. This page is for reference only.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; Simple breakout board for the 3.5mm audio jack. Use this breakout (shipped bare) to allow breadboard or SIP access to the super-common 3.5mm audio jack. All five pins are broken out.&lt;br /&gt;


	&lt;br /&gt;


	&lt;strong&gt;&lt;span style=&quot;font-weight: bold;&quot;&gt;Note: &lt;/span&gt;&lt;/strong&gt;This is for the bare PCB only.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Note:&lt;/strong&gt; The silkscreen is incorrect. We are working on a revision. However, the board is still usable, but the labeling isn&amp;#39;t even close to correct. Here is the correct pin labeling (from top to bottom):&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		GND (Ground)&lt;/li&gt;


	&lt;li&gt;


		RNG (Ring)&lt;/li&gt;


	&lt;li&gt;


		RSH (Ring Shunt)&lt;/li&gt;


	&lt;li&gt;


		TIP (Tip)&lt;/li&gt;


	&lt;li&gt;


		TSH (Tip Shunt)&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt; &lt;a href=&quot;http://www.sparkfun.com/datasheets/BreakoutBoards/audiojack_breakoutsch.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/p&gt;</description>
<title>Audio Jack Breakout</title>
<url>http://www.sparkfun.com/products/8827</url>
<tags>
<tag>Audio</tag>
</tags>
<properties>
<property name='family'>Audio Breakout</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/audiojack_breakout-v11_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/audiojack_breakout-v11_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/audiojack_breakout-v11_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/audiojack_breakout-v11_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector0pad'/><p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='male' name='RING_SHUNT'>
<description>RING_SHUNT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector1pad'/><p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
<connector id='connector2' type='male' name='RING'>
<description>RING</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector2pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector2pad'/><p layer='copper1' svgId='connector2pad'/></pcbView>
</views>
</connector>
<connector id='connector3' type='male' name='TIP_SHUNT'>
<description>TIP_SHUNT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector3pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector3pad'/><p layer='copper1' svgId='connector3pad'/></pcbView>
</views>
</connector>
<connector id='connector4' type='male' name='TIP'>
<description>TIP</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
