<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-PIC-ICSP-PTH">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' PIC-ICSP PTH -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>ISCP Programming connector for UAV, UBW Kit, etc.</description>
<title>PIC-ICSP</title>
<tags>
<tag>PTH</tag>
<tag>MOLEX-1X6</tag>
<tag>PIC-ICSP</tag>
</tags>
<properties>
<property name="package">molex-1x6</property>
<property name="family">sparkfun PIC ISCP</property>
<property name="connector">6 Pin</property>
<property name="variant">pth</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/generic_female_pin_header_6_100mil_bread.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_icsp-pic_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/molex_6_100mil_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/generic_female_pin_header_6_100mil_bread.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector3" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pin"/>
<p layer="copper1" svgId="connector3pin"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="PGC" type="male">
<description>PGC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pin"/>
<p layer="copper1" svgId="connector1pin"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="PGD" type="male">
<description>PGD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pin"/>
<p layer="copper1" svgId="connector2pin"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="PGM" type="male">
<description>PGM</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pin"/>
<p layer="copper1" svgId="connector0pin"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="VCC" type="male">
<description>VCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector4pin"/>
<p layer="copper1" svgId="connector4pin"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="VPP" type="male">
<description>VPP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector5pin"/>
<p layer="copper1" svgId="connector5pin"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>