<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.1b.02.04.5837" moduleId="8e4b4f3e54f56b3f712afc6a8e6a8a71">
    <version>4</version>
    <author>Fritzing Part-o-matic</author>
    <title>atmega168</title>
    <label>U</label>
    <date>2009-10-23</date>
    <tags>
        <tag>DIP</tag>
        <tag>ICt</tag>
        <tag>Microcontroller</tag>
        <tag>Atmel</tag>
        <tag>through-hole</tag>
    </tags>
    <properties>
        <property name="version">Atmega168-20PU</property>
        <property name="package">dip</property>
        <property name="family">Microcontroller</property>
        <property name="type">ATMEGA168</property>
		<property name="variant">dip28 THT</property>
		 
    </properties>
    <description>Atmel ATmega168 microcontroller.  The hardware hacker favorite.</description>
    <views>
        <iconView>
            <layers image="icon/microcontroller.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/atmega_breadboard_8e4b4f3e54f56b3f712afc6a8e6a8a71.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/atmega_schematic_8e4b4f3e54f56b3f712afc6a8e6a8a71.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/atmega_pcb_8e4b4f3e54f56b3f712afc6a8e6a8a71.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" type="male" name="D10 (PWM)">
            <description>pin 16</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector15pin"/>
                    <p layer="copper0" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="GND">
            <description>pin 8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="XLAT1">
            <description>pin 9</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" type="male" name="D11 (PWM)">
            <description>pin 17</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector16pin"/>
                    <p layer="copper0" svgId="connector16pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" type="male" name="D12">
            <description>pin 18</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector17pin"/>
                    <p layer="copper0" svgId="connector17pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="XLAT2">
            <description>pin 10</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" type="male" name="D13">
            <description>pin 19</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector18pin"/>
                    <p layer="copper0" svgId="connector18pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" type="male" name="AVCC">
            <description>pin 20</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector19pin"/>
                    <p layer="copper0" svgId="connector19pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" type="male" name="AREF">
            <description>pin 21</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector20pin"/>
                    <p layer="copper0" svgId="connector20pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" type="male" name="GND">
            <description>pin 22</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector21pin"/>
                    <p layer="copper0" svgId="connector21pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" type="male" name="A0">
            <description>pin 23</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector22pin"/>
                    <p layer="copper0" svgId="connector22pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" type="male" name="A1">
            <description>pin 24</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector23pin"/>
                    <p layer="copper0" svgId="connector23pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" type="male" name="A2">
            <description>pin 25</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin" terminalId="connector24terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector24pin"/>
                    <p layer="copper0" svgId="connector24pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector25" type="male" name="A3">
            <description>pin 26</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector25pin" terminalId="connector25terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector25pin"/>
                    <p layer="copper0" svgId="connector25pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" type="male" name="A4">
            <description>pin 27</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin" terminalId="connector26terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector26pin"/>
                    <p layer="copper0" svgId="connector26pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector27" type="male" name="A5">
            <description>pin 28</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector27pin" terminalId="connector27terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector27pin"/>
                    <p layer="copper0" svgId="connector27pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="RESET">
            <description>pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="D0 (RX)">
            <description>pin 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="D1 (TX)">
            <description>pin 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="D5 (PWM)">
            <description>pin 11</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="D2">
            <description>pin 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="D6 (PWM)">
            <description>pin 12</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin"/>
                    <p layer="copper0" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="D3 (PWM)">
            <description>pin 5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="D7">
            <description>pin 13</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin"/>
                    <p layer="copper0" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="D4">
            <description>pin 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="D8">
            <description>pin 14</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin"/>
                    <p layer="copper0" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="D9 (PWM)">
            <description>pin 15</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin"/>
                    <p layer="copper0" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="VCC">
            <description>pin 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
