<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module moduleId="AMT103_1" referenceFile="AMT103_1.fzp" fritzingVersion="0.9.3b">
  <version>4</version>
  <author>Nitay Megides Modified by vanepp July 2019</author>
  <title>AMT103</title>
  <label>CUI-enc</label>
  <date>Sat Jul 14 2018</date>
  <url>https://www.cui.com/product/resource/amt10.pdf</url>
  <tags>
    <tag>AMT</tag>
    <tag>Encoder</tag>
    <tag>FRC</tag>
  </tags>
  <properties>
    <property name="family">rotary encoders</property>
    <property name="editable pin labels">false</property>
    <property name="layer"/>
    <property name="part number"/>
    <property name="pins">5</property>
    <property name="pin spacing">100mil</property>
    <property name="variant">Variant 1</property>
  </properties>
  <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd"&gt;
&lt;html&gt;&lt;head&gt;&lt;meta name="qrichtext" content="1" /&gt;&lt;style type="text/css"&gt;
p, li { white-space: pre-wrap; }
&lt;/style&gt;&lt;/head&gt;&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;"&gt;
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;"&gt;CUI AMT103 Modular incremental encoder. Resolutions 48, 96, 100, 125, 192, 200, 250, 256, 384, 400, 500, 512, 800, 1000, 1024, 2048 either fixed (resolution indicated by part number) or selectable via dip switch. Index output once per revolution. VCC 5V (3.6V min, probably too high for 3.3V operation)&lt;/p&gt;&lt;/body&gt;&lt;/html&gt;</description>
  <views>
    <iconView>
      <layers image="icon/AMT103_1_icon.svg">
        <layer layerId="icon"/>
      </layers>
    </iconView>
    <breadboardView>
      <layers image="breadboard/AMT103_1_breadboard.svg">
        <layer layerId="breadboard"/>
      </layers>
    </breadboardView>
    <schematicView>
      <layers image="schematic/AMT103_1_schematic.svg">
        <layer layerId="schematic"/>
      </layers>
    </schematicView>
    <pcbView>
      <layers image="pcb/AMT103_1_pcb.svg">
        <layer layerId="silkscreen"/>
        <layer layerId="copper0"/>
        <layer layerId="copper1"/>
      </layers>
    </pcbView>
  </views>
  <connectors>
    <connector type="male" id="connector0" name="B">
      <description>B Channel quadrature output</description>
      <views>
        <breadboardView>
          <p svgId="connector0pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
        </schematicView>
        <pcbView>
          <p svgId="connector0pin" layer="copper0"/>
          <p svgId="connector0pin" layer="copper1"/>
        </pcbView>
      </views>
    </connector>
    <connector type="male" id="connector1" name="5V">
      <description>VCC (5V)</description>
      <views>
        <breadboardView>
          <p svgId="connector1pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
        </schematicView>
        <pcbView>
          <p svgId="connector1pin" layer="copper0"/>
          <p svgId="connector1pin" layer="copper1"/>
        </pcbView>
      </views>
    </connector>
    <connector type="male" id="connector2" name="A">
      <description>A Channel quadrature output</description>
      <views>
        <breadboardView>
          <p svgId="connector2pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
        </schematicView>
        <pcbView>
          <p svgId="connector2pin" layer="copper0"/>
          <p svgId="connector2pin" layer="copper1"/>
        </pcbView>
      </views>
    </connector>
    <connector type="male" id="connector3" name="X">
      <description>Index Channel Output (once per revolution)</description>
      <views>
        <breadboardView>
          <p svgId="connector3pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
        </schematicView>
        <pcbView>
          <p svgId="connector3pin" layer="copper0"/>
          <p svgId="connector3pin" layer="copper1"/>
        </pcbView>
      </views>
    </connector>
    <connector type="male" id="connector4" name="GND">
      <description>Ground</description>
      <views>
        <breadboardView>
          <p svgId="connector4pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
        </schematicView>
        <pcbView>
          <p svgId="connector4pin" layer="copper0"/>
          <p svgId="connector4pin" layer="copper1"/>
        </pcbView>
      </views>
    </connector>
  </connectors>
</module>
