<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.4.1b.07.17.4356" moduleId="ad901601e6d29266846fc9e4568504b6">
    <author>tigoe</author>
    <title>Barometric Pressure Sensor</title>
    <label>U</label>
    <date>2010-08-03</date>
    <tags>
        <tag>sensor</tag>
        <tag>pressure</tag>
        <tag>barometric</tag>
        <tag>breakout</tag>
    </tags>
    <properties>
        <property name="family">Pressure Sensors</property>
    </properties>
    <description>SCP1000 Barometric Pressure sensor.  Can sense air pressure and temperature.  SPI interface.</description>
    <views>
        <iconView>
            <layers image="icon/Barometric_Pressure_Sensor__2eaec138e035.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <schematicView>
            <layers image="schematic/Barometric_Pressure_Sensor__2eaec138e035.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <breadboardView>
            <layers image="breadboard/Barometric_Pressure_Sensor__2eaec138e035.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/jumper_7_100mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" name="MOSI" type="male">
            <description>Master Out, Slave In</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" name="SCK" type="male">
            <description>SPI Clock</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" name="3.3V" type="male">
            <description>3.3v voltage input</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" name="GND" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" name="DRDY" type="male">
            <description>Data Ready Pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="CSB" type="male">
            <description>Chip Select (or Slave Select, in SPI terms)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="MISO" type="male">
            <description>Master in, Slave Out</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>