<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module fritzingVersion="0.9.0b.04.10.5970" moduleId="IchigoJamT" referenceFile="IchigoJamT.fzp">
 <version>1</version>
 <author>Takeshi Sasaki</author>
 <title>IchigoJam T</title>
 <label>IchigoJam T</label>
 <date>Sat Dec 9 2017</date>
 <url>https://ichigojam.net/index-en.html</url>
 <tags>
  <tag>IchigoJam T</tag>
  <tag>LPC1114FDH28</tag>
  <tag>BASIC</tag>
  <tag>IchigoJam</tag>
  <tag>Kid's PC</tag>
 </tags>
 <properties>
  <property name="family">CPU board (IchigoJam T)</property>
  <property name="variant">rev 1</property>
  <property name="layer"></property>
  <property name="processor">NXP LPC1114FDH28</property>
  <property name="part number"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS UI Gothic'; font-size:9pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt;">IchigoJam T (IchigoJam means also strawberry jam)  is a low-power, low-cost single board computer development platform.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt;">As &amp;quot;Kid's PC&amp;quot;, it is developing for children's programming education.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt;">In this series, the BASIC language is activated just by turning on the power, and there is a feature that it can program immediately.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt;">Because it has I/O ports, it is easy to control electronic work, not limited to programs.&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/IchigoJamT_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/IchigoJamT_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/IchigoJamT_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/IchigoJamT_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="VIDEO1" type="male">
   <description>Video sync signal output</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector0terminal" svgId="connector0pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="VIDEO2" type="male">
   <description>Video image signal output</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector1terminal" svgId="connector1pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="IN1" type="male">
   <description>Digital input (IN1), Internal pull-up</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector2terminal" svgId="connector2pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" name="IN2" type="male">
   <description>Analog input (IN2, ANA2)</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector3terminal" svgId="connector3pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" name="IN3" type="male">
   <description>I2C_SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector4terminal" svgId="connector4pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" name="IN4" type="male">
   <description>Digital input (IN4), Internal pull-up</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector5terminal" svgId="connector5pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" name="VCC" type="male">
   <description>Analog power input 3.3V</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector6terminal" svgId="connector6pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" name="GND" type="male">
   <description>Analog ground input</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector7terminal" svgId="connector7pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" name="OUT1" type="male">
   <description>Digital output (OUT1)</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector8terminal" svgId="connector8pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" name="OUT2" type="male">
   <description>Digital output (OUT2, PWM2)</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector9terminal" svgId="connector9pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" name="OUT3" type="male">
   <description>Digital output (OUT3, PWM3)</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector10terminal" svgId="connector10pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" name="OUT4" type="male">
   <description>Digital output (OUT4, PWM4)</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector11terminal" svgId="connector11pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" name="BTN" type="male">
   <description>for Button, Wake-up interrupt</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector12terminal" svgId="connector12pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" name="LED" type="male">
   <description>LED</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector13terminal" svgId="connector13pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" name="RXD" type="male">
   <description>UART receive / input</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector14terminal" svgId="connector14pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" name="TXD" type="male">
   <description>UART transmission / output</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector15terminal" svgId="connector15pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector16" name="OUT6" type="male">
   <description>Digital output (OUT6)</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector16terminal" svgId="connector16pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector17" name="OUT5" type="male">
   <description>Digital output (OUT5, PWM5)</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector17terminal" svgId="connector17pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector18" name="XTAL2" type="male">
   <description>Crystal oscillator buffer output</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector18terminal" svgId="connector18pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector19" name="XTAL1" type="male">
   <description>Crystal oscillator clock input</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector19terminal" svgId="connector19pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector20" name="VCC" type="male">
   <description>Main power input</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector20terminal" svgId="connector20pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector21" name="GND" type="male">
   <description>Main ground input</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector21terminal" svgId="connector21pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector22" name="RESET" type="male">
   <description>Reset input</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector22terminal" svgId="connector22pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector23" name="ISP" type="male">
   <description>Firmware writing</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector23terminal" svgId="connector23pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector24" name="SOUND" type="male">
   <description>Sound output</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector24terminal" svgId="connector24pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector25" name="KBD2" type="male">
   <description>Keyboard DATA</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector25terminal" svgId="connector25pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector26" name="SCL" type="male">
   <description>I2C_SCL</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector26terminal" svgId="connector26pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector27" name="KBD1" type="male">
   <description>Keyboard CLK</description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector27terminal" svgId="connector27pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector28" name="5V" type="male">
   <description>for USB power</description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector28terminal" svgId="connector28pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector29" name="SDA" type="male">
   <description>I2C_SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector29terminal" svgId="connector29pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector30" name="SCL" type="male">
   <description>I2C_SCL</description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector30terminal" svgId="connector30pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector31" name="3.3V" type="male">
   <description>3.3V</description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector31terminal" svgId="connector31pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector32" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector32terminal" svgId="connector32pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="3V3">
   <nodeMember connectorId="connector6"/>
   <nodeMember connectorId="connector31"/>
   <nodeMember connectorId="connector20"/>
  </bus>
  <bus id="GND">
   <nodeMember connectorId="connector7"/>
   <nodeMember connectorId="connector32"/>
   <nodeMember connectorId="connector21"/>
  </bus>
  <bus id="SDA">
   <nodeMember connectorId="connector4"/>
   <nodeMember connectorId="connector29"/>
  </bus>
  <bus id="SCL">
   <nodeMember connectorId="connector30"/>
   <nodeMember connectorId="connector26"/>
  </bus>
 </buses>
</module>
