<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.0b.06.21.4282" moduleId="3661e4bbb7d863e04ccf7a9994dc65ff">
<version replacedby="Arduino-Fio-v22">4</version>
    <author>Andr&#233; Kn&#246;rig</author>
    <title>Arduino Fio</title>
    <label>Arduino</label>
    <date>2010-07-01</date>
    <tags>
        <tag>fritzing core</tag>
        <tag>arduino</tag>
        <tag>funnel</tag>
        <tag>microcontroller</tag>
        <tag>atmega</tag>
    </tags>
    <properties>
        <property name="family">//obsolete//Microcontroller Board (Arduino)</property>
        <property name="processor">ATmega</property>
        <property name="variant">Arduino Fio</property>
    </properties>
    <description>The Arduino Fio is a microcontroller board based on the ATmega328P runs at 3.3V and 8 MHz. It has 14 digital input/output pins (of which 6 can be used as PWM outputs), 8 analog inputs, an on-board resonator, a reset button, and holes for mounting pin headers. It has connections for a Lithium Polymer battery and includes a charge circuit over USB. An XBee socket is available on the bottom of the board.
The Arduino Fio is intended for wireless applications. The user can upload sketches with an a FTDI cable or Sparkfun breakout board. Additionally, by using a modified USB-to-XBee adaptor such as XBee Explorer USB, the user can upload sketches wirelessly. The board comes without pre-mounted headers, allowing the use of various types of connectors or direct soldering of wires.
The Arduino Fio was designed by Shigeru Kobayashi and SparkFun Electronics, and manufactured by SparkFunElectronics.

http://arduino.cc/en/Main/ArduinoBoardFio</description>
    <views>
        <iconView>
            <layers image="icon/Arduino_Fio.svg">
                <layer layerId="icon" />
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Arduino_Fio.svg">
                <layer layerId="breadboard" />
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Arduino_Fio.svg">
                <layer layerId="schematic" />
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Arduino_Fio.svg">
                <layer layerId="copper0" />
                <layer layerId="silkscreen" />
                <layer layerId="copper1" />
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" name="GND" replacedby="connector23" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector15pin" />
                    <p layer="copper0" svgId="connector15pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" name="A0" replacedby="A0" type="male">
            <description>Analog Input 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin" />
                    <p layer="copper0" svgId="connector7pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" name="D2" replacedby="D2" type="male">
            <description>Digital I/O 2 (External Interrupt)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector16pin" />
                    <p layer="copper0" svgId="connector16pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" name="DTR" replacedby="connector53" type="male">
            <description>Data Terminal Ready - Bring low to reset the microcontroller</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin" />
                    <p layer="copper0" svgId="connector8pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" name="D3" replacedby="D3 PWM" type="male">
            <description>Digital I/O 3 (PWM, External Interrupt)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector17pin" />
                    <p layer="copper0" svgId="connector17pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" name="TXO" replacedby="D1/TXO" type="male">
            <description>Serial Transmit (connected to DIN on XBee)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin" />
                    <p layer="copper0" svgId="connector9pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" name="D4" replacedby="D4" type="male">
            <description>Digital I/O 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector18pin" />
                    <p layer="copper0" svgId="connector18pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" name="D5" replacedby="D5 PWM" type="male">
            <description>Digital I/O 5 (PWM)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector19pin" />
                    <p layer="copper0" svgId="connector19pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" name="D6" replacedby="D6 PWM" type="male">
            <description>Digital I/O 6 (PWM)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector20pin" />
                    <p layer="copper0" svgId="connector20pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" name="D7" replacedby="D7" type="male">
            <description>Digital I/O 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector21pin" />
                    <p layer="copper0" svgId="connector21pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" name="D8" replacedby="D8" type="male">
            <description>Digital I/O 8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector22pin" />
                    <p layer="copper0" svgId="connector22pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" name="D9" replacedby="D9 PWM" type="male">
            <description>Digital I/O 9 (PWM)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector23pin" />
                    <p layer="copper0" svgId="connector23pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" name="D10" replacedby="D10 PWM/SS" type="male">
            <description>Digital I/O 10 (PWM, SPI SS)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin" terminalId="connector24terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector24pin" />
                    <p layer="copper0" svgId="connector24pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector25" name="D11" replacedby="D11 PWM/MOSI" type="male">
            <description>Digital I/O 11 (PWM, SPI MOSI)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector25pin" terminalId="connector25terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector25pin" />
                    <p layer="copper0" svgId="connector25pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" name="D12" replacedby="D12/MISO" type="male">
            <description>Digital I/O 12 (SPI MISO)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin" terminalId="connector26terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector26pin" />
                    <p layer="copper0" svgId="connector26pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector27" name="D13" replacedby="D13/SCK" type="male">
            <description>Digital I/O 13 (SPI SCK)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector27pin" terminalId="connector27terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector27pin" />
                    <p layer="copper0" svgId="connector27pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" name="A7" replacedby="A7" type="male">
            <description>Analog Input 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin" />
                    <p layer="copper0" svgId="connector0pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="A6" replacedby="A6" type="male">
            <description>Analog Input 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin" />
                    <p layer="copper0" svgId="connector1pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" name="RXI" replacedby="connector51" type="male">
            <description>Serial Receive (connected to DOUT on XBee)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin" />
                    <p layer="copper0" svgId="connector10pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="A5" replacedby="A5/SCL" type="male">
            <description>Analog Input 5 (I2C SCL)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin" />
                    <p layer="copper0" svgId="connector2pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" name="A4" replacedby="A4/SDA" type="male">
            <description>Analog Input 4 (I2C SDA)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin" />
                    <p layer="copper0" svgId="connector3pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" name="3V3" replacedby="connector50" type="male">
            <description>Power 3.3V</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin" />
                    <p layer="copper0" svgId="connector11pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" name="A3" replacedby="A3" type="male">
            <description>Analog Input 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin" />
                    <p layer="copper0" svgId="connector4pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" name="AREF" replacedby="AREF" type="male">
            <description>Reference voltage for analog input</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin" />
                    <p layer="copper0" svgId="connector12pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" name="A2" replacedby="A2" type="male">
            <description>Analog Input 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin" />
                    <p layer="copper0" svgId="connector5pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" name="GND" replacedby="connector48" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin" />
                    <p layer="copper0" svgId="connector13pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" name="A1" replacedby="A1" type="male">
            <description>Analog Input 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin" />
                    <p layer="copper0" svgId="connector6pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" name="3V3" replacedby="connector22" type="male">
            <description>Power (3.3V)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin" />
                    <p layer="copper0" svgId="connector14pin" />
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
      <bus id="ground">
       <nodeMember connectorId="connector13" />
       <nodeMember connectorId="connector15" />
      </bus>
      <bus id="3v3">
       <nodeMember connectorId="connector14" />
       <nodeMember connectorId="connector11" />
      </bus>
    </buses>
</module>