<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.18b.04.14.4111" moduleId="40a05d9dc2asdf9c6e50e467c97a50e">
 <version replacedby="stereo-jack-3_5mm">4</version>
    <author>Lionel Michel</author>
    <title>Stereo Jack (TRS) 3.5mm</title>
    <label>TRS</label>
    <date>2010-04-14</date>
    <tags>
        <tag>audio</tag>
        <tag>stereo</tag>
        <tag>jack</tag>
        <tag>connector</tag>
        <tag>sound</tag>
        <tag>tip ring sleeve</tag>
    </tags>
    <properties>
        <property name="package">PG203J [THT]</property>
        <property name="channels">Stereo</property>
        <property name="size">3.5 mm</property>
        <property name="family">//obsolete//Audio Connector</property>
    </properties>
    <description>Stereo Jack 3.5mm</description>
    <views>
        <iconView>
            <layers image="icon/stereo-jack-3_5mm.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/stereo-jack-3_5mm.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/stereo-jack-3_5mm.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/stereo-jack-3_5mm-PG203J.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" name="Tip" type="male">
            <description>usually left-hand audio channel</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                <p layer="copper1" svgId="connector3pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector4" name="Tip" type="male">
            <description>usually left-hand audio channel</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                <p layer="copper1" svgId="connector4pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector0" name="Sleeve" type="male">
            <description>usually ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="Ring" type="male">
            <description>usually right-hand audio channel</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="Ring" type="male">
            <description>usually right-hand audio channel</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
    <bus id="bus0">
		<nodeMember connectorId="connector1"/>
		<nodeMember connectorId="connector2"/>
	</bus>
	<bus id="bus1">
		<nodeMember connectorId="connector3"/>
		<nodeMember connectorId="connector4"/>
</bus>
</buses>
</module>