<?xml version="1.0" encoding="UTF-8"?><module moduleId="BreadboardModuleID" fritzingVersion="0.12.34">
 <version>4</version>
 <author>Dirk van Oosterbosch</author>
 <title>Generic Bajillion Hole Breadboard</title>
 <date>2008-12-08</date>
 <label>Breadboard</label>
 <tags>
  <tag>breadboard</tag>
 </tags>
 <properties>
  <property name="family">Breadboard</property>
  <property name="size">full</property>
 </properties>
 <taxonomy>prototyping.breadboard.breadboard.breadboard0</taxonomy>
 <description>A breadboard for easily prototyping circuits</description>
 <views>
  <iconView>
   <layers image="icon/breadboardicon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="breadboard/breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="breadboard/breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </pcbView>
 </views>
 <connectors ignoreTerminalPoints="true">
  <connector id="A98" name="A98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B98" name="B98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C98" name="C98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D98" name="D98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E98" name="E98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A99" name="A99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B99" name="B99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C99" name="C99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D99" name="D99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E99" name="E99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A1" name="A1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B1" name="B1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C1" name="C1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D1" name="D1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E1" name="E1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A2" name="A2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B2" name="B2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C2" name="C2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D2" name="D2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E2" name="E2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A3" name="A3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B3" name="B3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C3" name="C3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D3" name="D3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E3" name="E3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A4" name="A4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B4" name="B4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C4" name="C4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D4" name="D4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E4" name="E4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A5" name="A5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B5" name="B5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C5" name="C5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D5" name="D5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E5" name="E5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A6" name="A6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B6" name="B6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C6" name="C6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D6" name="D6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E6" name="E6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A7" name="A7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B7" name="B7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C7" name="C7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D7" name="D7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E7" name="E7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A8" name="A8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B8" name="B8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C8" name="C8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D8" name="D8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E8" name="E8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A9" name="A9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B9" name="B9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C9" name="C9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D9" name="D9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E9" name="E9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A10" name="A10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B10" name="B10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C10" name="C10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D10" name="D10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E10" name="E10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A11" name="A11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B11" name="B11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C11" name="C11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D11" name="D11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E11" name="E11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A12" name="A12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B12" name="B12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C12" name="C12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D12" name="D12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E12" name="E12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A13" name="A13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B13" name="B13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C13" name="C13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D13" name="D13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E13" name="E13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A14" name="A14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B14" name="B14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C14" name="C14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D14" name="D14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E14" name="E14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A15" name="A15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B15" name="B15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C15" name="C15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D15" name="D15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E15" name="E15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A16" name="A16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B16" name="B16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C16" name="C16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D16" name="D16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E16" name="E16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A17" name="A17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B17" name="B17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C17" name="C17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D17" name="D17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E17" name="E17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A18" name="A18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B18" name="B18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C18" name="C18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D18" name="D18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E18" name="E18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A19" name="A19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B19" name="B19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C19" name="C19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D19" name="D19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E19" name="E19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A20" name="A20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B20" name="B20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C20" name="C20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D20" name="D20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E20" name="E20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A21" name="A21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B21" name="B21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C21" name="C21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D21" name="D21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E21" name="E21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A22" name="A22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B22" name="B22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C22" name="C22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D22" name="D22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E22" name="E22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A23" name="A23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B23" name="B23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C23" name="C23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D23" name="D23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E23" name="E23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A24" name="A24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B24" name="B24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C24" name="C24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D24" name="D24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E24" name="E24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A25" name="A25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B25" name="B25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C25" name="C25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D25" name="D25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E25" name="E25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A26" name="A26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B26" name="B26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C26" name="C26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D26" name="D26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E26" name="E26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A27" name="A27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B27" name="B27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C27" name="C27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D27" name="D27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E27" name="E27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A28" name="A28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B28" name="B28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C28" name="C28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D28" name="D28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E28" name="E28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A29" name="A29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B29" name="B29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C29" name="C29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D29" name="D29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E29" name="E29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A30" name="A30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B30" name="B30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C30" name="C30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D30" name="D30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E30" name="E30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A31" name="A31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B31" name="B31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C31" name="C31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D31" name="D31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E31" name="E31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A32" name="A32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B32" name="B32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C32" name="C32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D32" name="D32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E32" name="E32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A33" name="A33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B33" name="B33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C33" name="C33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D33" name="D33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E33" name="E33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A34" name="A34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B34" name="B34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C34" name="C34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D34" name="D34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E34" name="E34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A35" name="A35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B35" name="B35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C35" name="C35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D35" name="D35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E35" name="E35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A36" name="A36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B36" name="B36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C36" name="C36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D36" name="D36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E36" name="E36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A37" name="A37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B37" name="B37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C37" name="C37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D37" name="D37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E37" name="E37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A38" name="A38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B38" name="B38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C38" name="C38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D38" name="D38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E38" name="E38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A39" name="A39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B39" name="B39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C39" name="C39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D39" name="D39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E39" name="E39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A40" name="A40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B40" name="B40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C40" name="C40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D40" name="D40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E40" name="E40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A41" name="A41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B41" name="B41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C41" name="C41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D41" name="D41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E41" name="E41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A42" name="A42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B42" name="B42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C42" name="C42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D42" name="D42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E42" name="E42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A43" name="A43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B43" name="B43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C43" name="C43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D43" name="D43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E43" name="E43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A44" name="A44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B44" name="B44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C44" name="C44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D44" name="D44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E44" name="E44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A45" name="A45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B45" name="B45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C45" name="C45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D45" name="D45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E45" name="E45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A46" name="A46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B46" name="B46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C46" name="C46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D46" name="D46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E46" name="E46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A47" name="A47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B47" name="B47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C47" name="C47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D47" name="D47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E47" name="E47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A48" name="A48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B48" name="B48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C48" name="C48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D48" name="D48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E48" name="E48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A49" name="A49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B49" name="B49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C49" name="C49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D49" name="D49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E49" name="E49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A50" name="A50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B50" name="B50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C50" name="C50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D50" name="D50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E50" name="E50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A51" name="A51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B51" name="B51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C51" name="C51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D51" name="D51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E51" name="E51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A52" name="A52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B52" name="B52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C52" name="C52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D52" name="D52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E52" name="E52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A53" name="A53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B53" name="B53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C53" name="C53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D53" name="D53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E53" name="E53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A54" name="A54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B54" name="B54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C54" name="C54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D54" name="D54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E54" name="E54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A55" name="A55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B55" name="B55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C55" name="C55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D55" name="D55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E55" name="E55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A56" name="A56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B56" name="B56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C56" name="C56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D56" name="D56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E56" name="E56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A57" name="A57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B57" name="B57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C57" name="C57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D57" name="D57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E57" name="E57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A58" name="A58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B58" name="B58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C58" name="C58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D58" name="D58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E58" name="E58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A59" name="A59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B59" name="B59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C59" name="C59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D59" name="D59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E59" name="E59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A60" name="A60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B60" name="B60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C60" name="C60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D60" name="D60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E60" name="E60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A61" name="A61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B61" name="B61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C61" name="C61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D61" name="D61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E61" name="E61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="A62" name="A62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="A62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="A62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="A62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="B62" name="B62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="B62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="B62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="B62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="C62" name="C62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="C62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="C62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="C62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="D62" name="D62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="D62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="D62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="D62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="E62" name="E62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="E62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="E62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="E62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F98" name="F98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G98" name="G98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H98" name="H98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I98" name="I98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J98" name="J98" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J98pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J98pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J98pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F99" name="F99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G99" name="G99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H99" name="H99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I99" name="I99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J99" name="J99" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J99pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J99pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J99pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F1" name="F1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G1" name="G1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H1" name="H1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I1" name="I1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J1" name="J1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F2" name="F2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G2" name="G2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H2" name="H2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I2" name="I2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J2" name="J2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F3" name="F3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G3" name="G3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H3" name="H3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I3" name="I3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J3" name="J3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F4" name="F4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G4" name="G4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H4" name="H4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I4" name="I4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J4" name="J4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F5" name="F5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G5" name="G5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H5" name="H5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I5" name="I5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J5" name="J5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F6" name="F6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G6" name="G6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H6" name="H6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I6" name="I6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J6" name="J6" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J6pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J6pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F7" name="F7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G7" name="G7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H7" name="H7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I7" name="I7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J7" name="J7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F8" name="F8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G8" name="G8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H8" name="H8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I8" name="I8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J8" name="J8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F9" name="F9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G9" name="G9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H9" name="H9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I9" name="I9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J9" name="J9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F10" name="F10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G10" name="G10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H10" name="H10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I10" name="I10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J10" name="J10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F11" name="F11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G11" name="G11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H11" name="H11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I11" name="I11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J11" name="J11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F12" name="F12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G12" name="G12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H12" name="H12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I12" name="I12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J12" name="J12" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J12pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J12pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F13" name="F13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G13" name="G13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H13" name="H13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I13" name="I13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J13" name="J13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F14" name="F14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G14" name="G14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H14" name="H14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I14" name="I14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J14" name="J14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F15" name="F15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G15" name="G15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H15" name="H15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I15" name="I15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J15" name="J15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F16" name="F16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G16" name="G16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H16" name="H16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I16" name="I16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J16" name="J16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F17" name="F17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G17" name="G17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H17" name="H17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I17" name="I17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J17" name="J17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F18" name="F18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G18" name="G18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H18" name="H18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I18" name="I18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J18" name="J18" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J18pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J18pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F19" name="F19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G19" name="G19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H19" name="H19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I19" name="I19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J19" name="J19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F20" name="F20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G20" name="G20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H20" name="H20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I20" name="I20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J20" name="J20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F21" name="F21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G21" name="G21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H21" name="H21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I21" name="I21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J21" name="J21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F22" name="F22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G22" name="G22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H22" name="H22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I22" name="I22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J22" name="J22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F23" name="F23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G23" name="G23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H23" name="H23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I23" name="I23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J23" name="J23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F24" name="F24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G24" name="G24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H24" name="H24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I24" name="I24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J24" name="J24" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J24pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J24pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F25" name="F25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G25" name="G25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H25" name="H25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I25" name="I25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J25" name="J25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F26" name="F26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G26" name="G26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H26" name="H26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I26" name="I26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J26" name="J26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F27" name="F27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G27" name="G27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H27" name="H27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I27" name="I27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J27" name="J27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F28" name="F28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G28" name="G28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H28" name="H28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I28" name="I28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J28" name="J28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F29" name="F29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G29" name="G29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H29" name="H29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I29" name="I29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J29" name="J29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F30" name="F30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G30" name="G30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H30" name="H30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I30" name="I30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J30" name="J30" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J30pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J30pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F31" name="F31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G31" name="G31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H31" name="H31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I31" name="I31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J31" name="J31" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J31pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J31pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F32" name="F32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G32" name="G32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H32" name="H32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I32" name="I32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J32" name="J32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F33" name="F33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G33" name="G33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H33" name="H33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I33" name="I33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J33" name="J33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F34" name="F34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G34" name="G34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H34" name="H34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I34" name="I34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J34" name="J34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F35" name="F35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G35" name="G35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H35" name="H35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I35" name="I35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J35" name="J35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F36" name="F36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G36" name="G36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H36" name="H36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I36" name="I36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J36" name="J36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F37" name="F37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G37" name="G37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H37" name="H37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I37" name="I37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J37" name="J37" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J37pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J37pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F38" name="F38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G38" name="G38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H38" name="H38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I38" name="I38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J38" name="J38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F39" name="F39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G39" name="G39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H39" name="H39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I39" name="I39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J39" name="J39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F40" name="F40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G40" name="G40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H40" name="H40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I40" name="I40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J40" name="J40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F41" name="F41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G41" name="G41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H41" name="H41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I41" name="I41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J41" name="J41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F42" name="F42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G42" name="G42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H42" name="H42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I42" name="I42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J42" name="J42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F43" name="F43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G43" name="G43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H43" name="H43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I43" name="I43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J43" name="J43" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J43pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J43pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F44" name="F44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G44" name="G44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H44" name="H44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I44" name="I44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J44" name="J44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F45" name="F45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G45" name="G45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H45" name="H45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I45" name="I45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J45" name="J45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F46" name="F46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G46" name="G46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H46" name="H46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I46" name="I46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J46" name="J46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F47" name="F47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G47" name="G47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H47" name="H47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I47" name="I47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J47" name="J47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F48" name="F48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G48" name="G48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H48" name="H48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I48" name="I48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J48" name="J48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F49" name="F49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G49" name="G49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H49" name="H49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I49" name="I49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J49" name="J49" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J49pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J49pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F50" name="F50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G50" name="G50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H50" name="H50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I50" name="I50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J50" name="J50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F51" name="F51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G51" name="G51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H51" name="H51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I51" name="I51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J51" name="J51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F52" name="F52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G52" name="G52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H52" name="H52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I52" name="I52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J52" name="J52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F53" name="F53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G53" name="G53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H53" name="H53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I53" name="I53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J53" name="J53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F54" name="F54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G54" name="G54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H54" name="H54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I54" name="I54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J54" name="J54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F55" name="F55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G55" name="G55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H55" name="H55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I55" name="I55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J55" name="J55" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J55pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J55pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F56" name="F56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G56" name="G56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H56" name="H56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I56" name="I56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J56" name="J56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F57" name="F57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G57" name="G57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H57" name="H57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I57" name="I57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J57" name="J57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F58" name="F58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G58" name="G58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H58" name="H58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I58" name="I58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J58" name="J58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F59" name="F59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G59" name="G59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H59" name="H59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I59" name="I59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J59" name="J59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F60" name="F60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G60" name="G60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H60" name="H60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I60" name="I60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J60" name="J60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F61" name="F61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G61" name="G61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H61" name="H61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I61" name="I61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J61" name="J61" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J61pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J61pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="F62" name="F62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="F62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="F62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="F62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="G62" name="G62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="G62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="G62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="G62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="H62" name="H62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="H62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="H62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="H62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="I62" name="I62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="I62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="I62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="I62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="J62" name="J62" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="J62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="J62pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="J62pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W1" name="W1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W2" name="W2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W3" name="W3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W4" name="W4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W5" name="W5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W7" name="W7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W8" name="W8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W9" name="W9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W10" name="W10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W11" name="W11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W13" name="W13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W14" name="W14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W15" name="W15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W16" name="W16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W17" name="W17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W19" name="W19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W20" name="W20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W21" name="W21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W22" name="W22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W23" name="W23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W25" name="W25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W26" name="W26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W27" name="W27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W28" name="W28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W29" name="W29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W32" name="W32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W33" name="W33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W34" name="W34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W35" name="W35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W36" name="W36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W38" name="W38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W39" name="W39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W40" name="W40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W41" name="W41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W42" name="W42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W44" name="W44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W45" name="W45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W46" name="W46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W47" name="W47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W48" name="W48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W50" name="W50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W51" name="W51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W52" name="W52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W53" name="W53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W54" name="W54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W56" name="W56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W57" name="W57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W58" name="W58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W59" name="W59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="W60" name="W60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="W60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="W60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="W60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X1" name="X1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X2" name="X2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X3" name="X3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X4" name="X4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X5" name="X5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X7" name="X7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X8" name="X8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X9" name="X9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X10" name="X10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X11" name="X11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X13" name="X13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X14" name="X14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X15" name="X15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X16" name="X16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X17" name="X17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X19" name="X19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X20" name="X20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X21" name="X21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X22" name="X22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X23" name="X23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X25" name="X25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X26" name="X26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X27" name="X27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X28" name="X28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X29" name="X29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X32" name="X32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X33" name="X33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X34" name="X34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X35" name="X35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X36" name="X36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X38" name="X38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X39" name="X39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X40" name="X40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X41" name="X41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X42" name="X42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X44" name="X44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X45" name="X45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X46" name="X46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X47" name="X47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X48" name="X48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X50" name="X50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X51" name="X51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X52" name="X52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X53" name="X53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X54" name="X54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X56" name="X56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X57" name="X57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X58" name="X58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X59" name="X59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="X60" name="X60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="X60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="X60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="X60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y1" name="Y1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y2" name="Y2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y3" name="Y3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y4" name="Y4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y5" name="Y5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y7" name="Y7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y8" name="Y8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y9" name="Y9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y10" name="Y10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y11" name="Y11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y13" name="Y13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y14" name="Y14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y15" name="Y15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y16" name="Y16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y17" name="Y17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y19" name="Y19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y20" name="Y20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y21" name="Y21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y22" name="Y22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y23" name="Y23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y25" name="Y25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y26" name="Y26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y27" name="Y27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y28" name="Y28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y29" name="Y29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y32" name="Y32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y33" name="Y33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y34" name="Y34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y35" name="Y35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y36" name="Y36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y38" name="Y38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y39" name="Y39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y40" name="Y40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y41" name="Y41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y42" name="Y42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y44" name="Y44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y45" name="Y45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y46" name="Y46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y47" name="Y47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y48" name="Y48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y50" name="Y50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y51" name="Y51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y52" name="Y52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y53" name="Y53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y54" name="Y54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y56" name="Y56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y57" name="Y57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y58" name="Y58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y59" name="Y59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Y60" name="Y60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Y60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Y60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Y60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z1" name="Z1" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z1pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z1pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z2" name="Z2" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z2pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z2pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z3" name="Z3" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z3pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z3pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z4" name="Z4" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z4pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z4pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z5" name="Z5" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z5pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z5pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z7" name="Z7" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z7pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z7pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z8" name="Z8" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z8pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z8pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z9" name="Z9" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z9pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z9pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z10" name="Z10" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z10pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z10pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z11" name="Z11" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z11pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z11pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z13" name="Z13" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z13pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z13pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z14" name="Z14" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z14pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z14pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z15" name="Z15" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z15pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z15pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z16" name="Z16" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z16pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z16pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z17" name="Z17" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z17pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z17pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z19" name="Z19" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z19pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z19pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z20" name="Z20" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z20pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z20pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z21" name="Z21" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z21pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z21pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z22" name="Z22" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z22pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z22pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z23" name="Z23" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z23pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z23pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z25" name="Z25" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z25pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z25pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z26" name="Z26" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z26pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z26pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z27" name="Z27" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z27pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z27pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z28" name="Z28" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z28pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z28pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z29" name="Z29" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z29pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z29pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z32" name="Z32" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z32pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z32pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z33" name="Z33" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z33pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z33pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z34" name="Z34" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z34pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z34pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z35" name="Z35" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z35pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z35pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z36" name="Z36" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z36pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z36pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z38" name="Z38" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z38pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z38pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z39" name="Z39" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z39pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z39pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z40" name="Z40" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z40pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z40pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z41" name="Z41" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z41pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z41pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z42" name="Z42" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z42pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z42pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z44" name="Z44" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z44pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z44pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z45" name="Z45" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z45pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z45pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z46" name="Z46" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z46pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z46pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z47" name="Z47" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z47pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z47pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z48" name="Z48" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z48pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z48pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z50" name="Z50" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z50pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z50pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z51" name="Z51" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z51pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z51pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z52" name="Z52" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z52pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z52pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z53" name="Z53" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z53pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z53pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z54" name="Z54" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z54pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z54pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z56" name="Z56" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z56pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z56pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z57" name="Z57" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z57pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z57pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z58" name="Z58" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z58pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z58pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z59" name="Z59" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z59pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z59pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
  <connector id="Z60" name="Z60" type="female">
   <description>breadboard socket</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="Z60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="breadboardbreadboard" svgId="Z60pin"/>
    </schematicView>
    <pcbView>
     <p layer="breadboardbreadboard" svgId="Z60pin"/>
    </pcbView>
   </views>
  <erc ignore="always"/></connector>
 </connectors>
 <buses>
  <bus id="bus0-4">
   <nodeMember connectorId="A98"/>
   <nodeMember connectorId="B98"/>
   <nodeMember connectorId="C98"/>
   <nodeMember connectorId="D98"/>
   <nodeMember connectorId="E98"/>
  </bus>
  <bus id="bus1-4">
   <nodeMember connectorId="A99"/>
   <nodeMember connectorId="B99"/>
   <nodeMember connectorId="C99"/>
   <nodeMember connectorId="D99"/>
   <nodeMember connectorId="E99"/>
  </bus>
  <bus id="bus2-4">
   <nodeMember connectorId="A1"/>
   <nodeMember connectorId="B1"/>
   <nodeMember connectorId="C1"/>
   <nodeMember connectorId="D1"/>
   <nodeMember connectorId="E1"/>
  </bus>
  <bus id="bus3-4">
   <nodeMember connectorId="A2"/>
   <nodeMember connectorId="B2"/>
   <nodeMember connectorId="C2"/>
   <nodeMember connectorId="D2"/>
   <nodeMember connectorId="E2"/>
  </bus>
  <bus id="bus4-4">
   <nodeMember connectorId="A3"/>
   <nodeMember connectorId="B3"/>
   <nodeMember connectorId="C3"/>
   <nodeMember connectorId="D3"/>
   <nodeMember connectorId="E3"/>
  </bus>
  <bus id="bus5-4">
   <nodeMember connectorId="A4"/>
   <nodeMember connectorId="B4"/>
   <nodeMember connectorId="C4"/>
   <nodeMember connectorId="D4"/>
   <nodeMember connectorId="E4"/>
  </bus>
  <bus id="bus6-4">
   <nodeMember connectorId="A5"/>
   <nodeMember connectorId="B5"/>
   <nodeMember connectorId="C5"/>
   <nodeMember connectorId="D5"/>
   <nodeMember connectorId="E5"/>
  </bus>
  <bus id="bus7-4">
   <nodeMember connectorId="A6"/>
   <nodeMember connectorId="B6"/>
   <nodeMember connectorId="C6"/>
   <nodeMember connectorId="D6"/>
   <nodeMember connectorId="E6"/>
  </bus>
  <bus id="bus8-4">
   <nodeMember connectorId="A7"/>
   <nodeMember connectorId="B7"/>
   <nodeMember connectorId="C7"/>
   <nodeMember connectorId="D7"/>
   <nodeMember connectorId="E7"/>
  </bus>
  <bus id="bus9-4">
   <nodeMember connectorId="A8"/>
   <nodeMember connectorId="B8"/>
   <nodeMember connectorId="C8"/>
   <nodeMember connectorId="D8"/>
   <nodeMember connectorId="E8"/>
  </bus>
  <bus id="bus10-4">
   <nodeMember connectorId="A9"/>
   <nodeMember connectorId="B9"/>
   <nodeMember connectorId="C9"/>
   <nodeMember connectorId="D9"/>
   <nodeMember connectorId="E9"/>
  </bus>
  <bus id="bus11-4">
   <nodeMember connectorId="A10"/>
   <nodeMember connectorId="B10"/>
   <nodeMember connectorId="C10"/>
   <nodeMember connectorId="D10"/>
   <nodeMember connectorId="E10"/>
  </bus>
  <bus id="bus12-4">
   <nodeMember connectorId="A11"/>
   <nodeMember connectorId="B11"/>
   <nodeMember connectorId="C11"/>
   <nodeMember connectorId="D11"/>
   <nodeMember connectorId="E11"/>
  </bus>
  <bus id="bus13-4">
   <nodeMember connectorId="A12"/>
   <nodeMember connectorId="B12"/>
   <nodeMember connectorId="C12"/>
   <nodeMember connectorId="D12"/>
   <nodeMember connectorId="E12"/>
  </bus>
  <bus id="bus14-4">
   <nodeMember connectorId="A13"/>
   <nodeMember connectorId="B13"/>
   <nodeMember connectorId="C13"/>
   <nodeMember connectorId="D13"/>
   <nodeMember connectorId="E13"/>
  </bus>
  <bus id="bus15-4">
   <nodeMember connectorId="A14"/>
   <nodeMember connectorId="B14"/>
   <nodeMember connectorId="C14"/>
   <nodeMember connectorId="D14"/>
   <nodeMember connectorId="E14"/>
  </bus>
  <bus id="bus16-4">
   <nodeMember connectorId="A15"/>
   <nodeMember connectorId="B15"/>
   <nodeMember connectorId="C15"/>
   <nodeMember connectorId="D15"/>
   <nodeMember connectorId="E15"/>
  </bus>
  <bus id="bus17-4">
   <nodeMember connectorId="A16"/>
   <nodeMember connectorId="B16"/>
   <nodeMember connectorId="C16"/>
   <nodeMember connectorId="D16"/>
   <nodeMember connectorId="E16"/>
  </bus>
  <bus id="bus18-4">
   <nodeMember connectorId="A17"/>
   <nodeMember connectorId="B17"/>
   <nodeMember connectorId="C17"/>
   <nodeMember connectorId="D17"/>
   <nodeMember connectorId="E17"/>
  </bus>
  <bus id="bus19-4">
   <nodeMember connectorId="A18"/>
   <nodeMember connectorId="B18"/>
   <nodeMember connectorId="C18"/>
   <nodeMember connectorId="D18"/>
   <nodeMember connectorId="E18"/>
  </bus>
  <bus id="bus20-4">
   <nodeMember connectorId="A19"/>
   <nodeMember connectorId="B19"/>
   <nodeMember connectorId="C19"/>
   <nodeMember connectorId="D19"/>
   <nodeMember connectorId="E19"/>
  </bus>
  <bus id="bus21-4">
   <nodeMember connectorId="A20"/>
   <nodeMember connectorId="B20"/>
   <nodeMember connectorId="C20"/>
   <nodeMember connectorId="D20"/>
   <nodeMember connectorId="E20"/>
  </bus>
  <bus id="bus22-4">
   <nodeMember connectorId="A21"/>
   <nodeMember connectorId="B21"/>
   <nodeMember connectorId="C21"/>
   <nodeMember connectorId="D21"/>
   <nodeMember connectorId="E21"/>
  </bus>
  <bus id="bus23-4">
   <nodeMember connectorId="A22"/>
   <nodeMember connectorId="B22"/>
   <nodeMember connectorId="C22"/>
   <nodeMember connectorId="D22"/>
   <nodeMember connectorId="E22"/>
  </bus>
  <bus id="bus24-4">
   <nodeMember connectorId="A23"/>
   <nodeMember connectorId="B23"/>
   <nodeMember connectorId="C23"/>
   <nodeMember connectorId="D23"/>
   <nodeMember connectorId="E23"/>
  </bus>
  <bus id="bus25-4">
   <nodeMember connectorId="A24"/>
   <nodeMember connectorId="B24"/>
   <nodeMember connectorId="C24"/>
   <nodeMember connectorId="D24"/>
   <nodeMember connectorId="E24"/>
  </bus>
  <bus id="bus26-4">
   <nodeMember connectorId="A25"/>
   <nodeMember connectorId="B25"/>
   <nodeMember connectorId="C25"/>
   <nodeMember connectorId="D25"/>
   <nodeMember connectorId="E25"/>
  </bus>
  <bus id="bus27-4">
   <nodeMember connectorId="A26"/>
   <nodeMember connectorId="B26"/>
   <nodeMember connectorId="C26"/>
   <nodeMember connectorId="D26"/>
   <nodeMember connectorId="E26"/>
  </bus>
  <bus id="bus28-4">
   <nodeMember connectorId="A27"/>
   <nodeMember connectorId="B27"/>
   <nodeMember connectorId="C27"/>
   <nodeMember connectorId="D27"/>
   <nodeMember connectorId="E27"/>
  </bus>
  <bus id="bus29-4">
   <nodeMember connectorId="A28"/>
   <nodeMember connectorId="B28"/>
   <nodeMember connectorId="C28"/>
   <nodeMember connectorId="D28"/>
   <nodeMember connectorId="E28"/>
  </bus>
  <bus id="bus30-4">
   <nodeMember connectorId="A29"/>
   <nodeMember connectorId="B29"/>
   <nodeMember connectorId="C29"/>
   <nodeMember connectorId="D29"/>
   <nodeMember connectorId="E29"/>
  </bus>
  <bus id="bus31-4">
   <nodeMember connectorId="A30"/>
   <nodeMember connectorId="B30"/>
   <nodeMember connectorId="C30"/>
   <nodeMember connectorId="D30"/>
   <nodeMember connectorId="E30"/>
  </bus>
  <bus id="bus32-4">
   <nodeMember connectorId="A31"/>
   <nodeMember connectorId="B31"/>
   <nodeMember connectorId="C31"/>
   <nodeMember connectorId="D31"/>
   <nodeMember connectorId="E31"/>
  </bus>
  <bus id="bus33-4">
   <nodeMember connectorId="A32"/>
   <nodeMember connectorId="B32"/>
   <nodeMember connectorId="C32"/>
   <nodeMember connectorId="D32"/>
   <nodeMember connectorId="E32"/>
  </bus>
  <bus id="bus34-4">
   <nodeMember connectorId="A33"/>
   <nodeMember connectorId="B33"/>
   <nodeMember connectorId="C33"/>
   <nodeMember connectorId="D33"/>
   <nodeMember connectorId="E33"/>
  </bus>
  <bus id="bus35-4">
   <nodeMember connectorId="A34"/>
   <nodeMember connectorId="B34"/>
   <nodeMember connectorId="C34"/>
   <nodeMember connectorId="D34"/>
   <nodeMember connectorId="E34"/>
  </bus>
  <bus id="bus36-4">
   <nodeMember connectorId="A35"/>
   <nodeMember connectorId="B35"/>
   <nodeMember connectorId="C35"/>
   <nodeMember connectorId="D35"/>
   <nodeMember connectorId="E35"/>
  </bus>
  <bus id="bus37-4">
   <nodeMember connectorId="A36"/>
   <nodeMember connectorId="B36"/>
   <nodeMember connectorId="C36"/>
   <nodeMember connectorId="D36"/>
   <nodeMember connectorId="E36"/>
  </bus>
  <bus id="bus38-4">
   <nodeMember connectorId="A37"/>
   <nodeMember connectorId="B37"/>
   <nodeMember connectorId="C37"/>
   <nodeMember connectorId="D37"/>
   <nodeMember connectorId="E37"/>
  </bus>
  <bus id="bus39-4">
   <nodeMember connectorId="A38"/>
   <nodeMember connectorId="B38"/>
   <nodeMember connectorId="C38"/>
   <nodeMember connectorId="D38"/>
   <nodeMember connectorId="E38"/>
  </bus>
  <bus id="bus40-4">
   <nodeMember connectorId="A39"/>
   <nodeMember connectorId="B39"/>
   <nodeMember connectorId="C39"/>
   <nodeMember connectorId="D39"/>
   <nodeMember connectorId="E39"/>
  </bus>
  <bus id="bus41-4">
   <nodeMember connectorId="A40"/>
   <nodeMember connectorId="B40"/>
   <nodeMember connectorId="C40"/>
   <nodeMember connectorId="D40"/>
   <nodeMember connectorId="E40"/>
  </bus>
  <bus id="bus42-4">
   <nodeMember connectorId="A41"/>
   <nodeMember connectorId="B41"/>
   <nodeMember connectorId="C41"/>
   <nodeMember connectorId="D41"/>
   <nodeMember connectorId="E41"/>
  </bus>
  <bus id="bus43-4">
   <nodeMember connectorId="A42"/>
   <nodeMember connectorId="B42"/>
   <nodeMember connectorId="C42"/>
   <nodeMember connectorId="D42"/>
   <nodeMember connectorId="E42"/>
  </bus>
  <bus id="bus44-4">
   <nodeMember connectorId="A43"/>
   <nodeMember connectorId="B43"/>
   <nodeMember connectorId="C43"/>
   <nodeMember connectorId="D43"/>
   <nodeMember connectorId="E43"/>
  </bus>
  <bus id="bus45-4">
   <nodeMember connectorId="A44"/>
   <nodeMember connectorId="B44"/>
   <nodeMember connectorId="C44"/>
   <nodeMember connectorId="D44"/>
   <nodeMember connectorId="E44"/>
  </bus>
  <bus id="bus46-4">
   <nodeMember connectorId="A45"/>
   <nodeMember connectorId="B45"/>
   <nodeMember connectorId="C45"/>
   <nodeMember connectorId="D45"/>
   <nodeMember connectorId="E45"/>
  </bus>
  <bus id="bus47-4">
   <nodeMember connectorId="A46"/>
   <nodeMember connectorId="B46"/>
   <nodeMember connectorId="C46"/>
   <nodeMember connectorId="D46"/>
   <nodeMember connectorId="E46"/>
  </bus>
  <bus id="bus48-4">
   <nodeMember connectorId="A47"/>
   <nodeMember connectorId="B47"/>
   <nodeMember connectorId="C47"/>
   <nodeMember connectorId="D47"/>
   <nodeMember connectorId="E47"/>
  </bus>
  <bus id="bus49-4">
   <nodeMember connectorId="A48"/>
   <nodeMember connectorId="B48"/>
   <nodeMember connectorId="C48"/>
   <nodeMember connectorId="D48"/>
   <nodeMember connectorId="E48"/>
  </bus>
  <bus id="bus50-4">
   <nodeMember connectorId="A49"/>
   <nodeMember connectorId="B49"/>
   <nodeMember connectorId="C49"/>
   <nodeMember connectorId="D49"/>
   <nodeMember connectorId="E49"/>
  </bus>
  <bus id="bus51-4">
   <nodeMember connectorId="A50"/>
   <nodeMember connectorId="B50"/>
   <nodeMember connectorId="C50"/>
   <nodeMember connectorId="D50"/>
   <nodeMember connectorId="E50"/>
  </bus>
  <bus id="bus52-4">
   <nodeMember connectorId="A51"/>
   <nodeMember connectorId="B51"/>
   <nodeMember connectorId="C51"/>
   <nodeMember connectorId="D51"/>
   <nodeMember connectorId="E51"/>
  </bus>
  <bus id="bus53-4">
   <nodeMember connectorId="A52"/>
   <nodeMember connectorId="B52"/>
   <nodeMember connectorId="C52"/>
   <nodeMember connectorId="D52"/>
   <nodeMember connectorId="E52"/>
  </bus>
  <bus id="bus54-4">
   <nodeMember connectorId="A53"/>
   <nodeMember connectorId="B53"/>
   <nodeMember connectorId="C53"/>
   <nodeMember connectorId="D53"/>
   <nodeMember connectorId="E53"/>
  </bus>
  <bus id="bus55-4">
   <nodeMember connectorId="A54"/>
   <nodeMember connectorId="B54"/>
   <nodeMember connectorId="C54"/>
   <nodeMember connectorId="D54"/>
   <nodeMember connectorId="E54"/>
  </bus>
  <bus id="bus56-4">
   <nodeMember connectorId="A55"/>
   <nodeMember connectorId="B55"/>
   <nodeMember connectorId="C55"/>
   <nodeMember connectorId="D55"/>
   <nodeMember connectorId="E55"/>
  </bus>
  <bus id="bus57-4">
   <nodeMember connectorId="A56"/>
   <nodeMember connectorId="B56"/>
   <nodeMember connectorId="C56"/>
   <nodeMember connectorId="D56"/>
   <nodeMember connectorId="E56"/>
  </bus>
  <bus id="bus58-4">
   <nodeMember connectorId="A57"/>
   <nodeMember connectorId="B57"/>
   <nodeMember connectorId="C57"/>
   <nodeMember connectorId="D57"/>
   <nodeMember connectorId="E57"/>
  </bus>
  <bus id="bus59-4">
   <nodeMember connectorId="A58"/>
   <nodeMember connectorId="B58"/>
   <nodeMember connectorId="C58"/>
   <nodeMember connectorId="D58"/>
   <nodeMember connectorId="E58"/>
  </bus>
  <bus id="bus60-4">
   <nodeMember connectorId="A59"/>
   <nodeMember connectorId="B59"/>
   <nodeMember connectorId="C59"/>
   <nodeMember connectorId="D59"/>
   <nodeMember connectorId="E59"/>
  </bus>
  <bus id="bus61-4">
   <nodeMember connectorId="A60"/>
   <nodeMember connectorId="B60"/>
   <nodeMember connectorId="C60"/>
   <nodeMember connectorId="D60"/>
   <nodeMember connectorId="E60"/>
  </bus>
  <bus id="bus62-4">
   <nodeMember connectorId="A61"/>
   <nodeMember connectorId="B61"/>
   <nodeMember connectorId="C61"/>
   <nodeMember connectorId="D61"/>
   <nodeMember connectorId="E61"/>
  </bus>
  <bus id="bus63-4">
   <nodeMember connectorId="A62"/>
   <nodeMember connectorId="B62"/>
   <nodeMember connectorId="C62"/>
   <nodeMember connectorId="D62"/>
   <nodeMember connectorId="E62"/>
  </bus>
  <bus id="bus0-11">
   <nodeMember connectorId="F98"/>
   <nodeMember connectorId="G98"/>
   <nodeMember connectorId="H98"/>
   <nodeMember connectorId="I98"/>
   <nodeMember connectorId="J98"/>
  </bus>
  <bus id="bus1-11">
   <nodeMember connectorId="F99"/>
   <nodeMember connectorId="G99"/>
   <nodeMember connectorId="H99"/>
   <nodeMember connectorId="I99"/>
   <nodeMember connectorId="J99"/>
  </bus>
  <bus id="bus2-11">
   <nodeMember connectorId="F1"/>
   <nodeMember connectorId="G1"/>
   <nodeMember connectorId="H1"/>
   <nodeMember connectorId="I1"/>
   <nodeMember connectorId="J1"/>
  </bus>
  <bus id="bus3-11">
   <nodeMember connectorId="F2"/>
   <nodeMember connectorId="G2"/>
   <nodeMember connectorId="H2"/>
   <nodeMember connectorId="I2"/>
   <nodeMember connectorId="J2"/>
  </bus>
  <bus id="bus4-11">
   <nodeMember connectorId="F3"/>
   <nodeMember connectorId="G3"/>
   <nodeMember connectorId="H3"/>
   <nodeMember connectorId="I3"/>
   <nodeMember connectorId="J3"/>
  </bus>
  <bus id="bus5-11">
   <nodeMember connectorId="F4"/>
   <nodeMember connectorId="G4"/>
   <nodeMember connectorId="H4"/>
   <nodeMember connectorId="I4"/>
   <nodeMember connectorId="J4"/>
  </bus>
  <bus id="bus6-11">
   <nodeMember connectorId="F5"/>
   <nodeMember connectorId="G5"/>
   <nodeMember connectorId="H5"/>
   <nodeMember connectorId="I5"/>
   <nodeMember connectorId="J5"/>
  </bus>
  <bus id="bus7-11">
   <nodeMember connectorId="F6"/>
   <nodeMember connectorId="G6"/>
   <nodeMember connectorId="H6"/>
   <nodeMember connectorId="I6"/>
   <nodeMember connectorId="J6"/>
  </bus>
  <bus id="bus8-11">
   <nodeMember connectorId="F7"/>
   <nodeMember connectorId="G7"/>
   <nodeMember connectorId="H7"/>
   <nodeMember connectorId="I7"/>
   <nodeMember connectorId="J7"/>
  </bus>
  <bus id="bus9-11">
   <nodeMember connectorId="F8"/>
   <nodeMember connectorId="G8"/>
   <nodeMember connectorId="H8"/>
   <nodeMember connectorId="I8"/>
   <nodeMember connectorId="J8"/>
  </bus>
  <bus id="bus10-11">
   <nodeMember connectorId="F9"/>
   <nodeMember connectorId="G9"/>
   <nodeMember connectorId="H9"/>
   <nodeMember connectorId="I9"/>
   <nodeMember connectorId="J9"/>
  </bus>
  <bus id="bus11-11">
   <nodeMember connectorId="F10"/>
   <nodeMember connectorId="G10"/>
   <nodeMember connectorId="H10"/>
   <nodeMember connectorId="I10"/>
   <nodeMember connectorId="J10"/>
  </bus>
  <bus id="bus12-11">
   <nodeMember connectorId="F11"/>
   <nodeMember connectorId="G11"/>
   <nodeMember connectorId="H11"/>
   <nodeMember connectorId="I11"/>
   <nodeMember connectorId="J11"/>
  </bus>
  <bus id="bus13-11">
   <nodeMember connectorId="F12"/>
   <nodeMember connectorId="G12"/>
   <nodeMember connectorId="H12"/>
   <nodeMember connectorId="I12"/>
   <nodeMember connectorId="J12"/>
  </bus>
  <bus id="bus14-11">
   <nodeMember connectorId="F13"/>
   <nodeMember connectorId="G13"/>
   <nodeMember connectorId="H13"/>
   <nodeMember connectorId="I13"/>
   <nodeMember connectorId="J13"/>
  </bus>
  <bus id="bus15-11">
   <nodeMember connectorId="F14"/>
   <nodeMember connectorId="G14"/>
   <nodeMember connectorId="H14"/>
   <nodeMember connectorId="I14"/>
   <nodeMember connectorId="J14"/>
  </bus>
  <bus id="bus16-11">
   <nodeMember connectorId="F15"/>
   <nodeMember connectorId="G15"/>
   <nodeMember connectorId="H15"/>
   <nodeMember connectorId="I15"/>
   <nodeMember connectorId="J15"/>
  </bus>
  <bus id="bus17-11">
   <nodeMember connectorId="F16"/>
   <nodeMember connectorId="G16"/>
   <nodeMember connectorId="H16"/>
   <nodeMember connectorId="I16"/>
   <nodeMember connectorId="J16"/>
  </bus>
  <bus id="bus18-11">
   <nodeMember connectorId="F17"/>
   <nodeMember connectorId="G17"/>
   <nodeMember connectorId="H17"/>
   <nodeMember connectorId="I17"/>
   <nodeMember connectorId="J17"/>
  </bus>
  <bus id="bus19-11">
   <nodeMember connectorId="F18"/>
   <nodeMember connectorId="G18"/>
   <nodeMember connectorId="H18"/>
   <nodeMember connectorId="I18"/>
   <nodeMember connectorId="J18"/>
  </bus>
  <bus id="bus20-11">
   <nodeMember connectorId="F19"/>
   <nodeMember connectorId="G19"/>
   <nodeMember connectorId="H19"/>
   <nodeMember connectorId="I19"/>
   <nodeMember connectorId="J19"/>
  </bus>
  <bus id="bus21-11">
   <nodeMember connectorId="F20"/>
   <nodeMember connectorId="G20"/>
   <nodeMember connectorId="H20"/>
   <nodeMember connectorId="I20"/>
   <nodeMember connectorId="J20"/>
  </bus>
  <bus id="bus22-11">
   <nodeMember connectorId="F21"/>
   <nodeMember connectorId="G21"/>
   <nodeMember connectorId="H21"/>
   <nodeMember connectorId="I21"/>
   <nodeMember connectorId="J21"/>
  </bus>
  <bus id="bus23-11">
   <nodeMember connectorId="F22"/>
   <nodeMember connectorId="G22"/>
   <nodeMember connectorId="H22"/>
   <nodeMember connectorId="I22"/>
   <nodeMember connectorId="J22"/>
  </bus>
  <bus id="bus24-11">
   <nodeMember connectorId="F23"/>
   <nodeMember connectorId="G23"/>
   <nodeMember connectorId="H23"/>
   <nodeMember connectorId="I23"/>
   <nodeMember connectorId="J23"/>
  </bus>
  <bus id="bus25-11">
   <nodeMember connectorId="F24"/>
   <nodeMember connectorId="G24"/>
   <nodeMember connectorId="H24"/>
   <nodeMember connectorId="I24"/>
   <nodeMember connectorId="J24"/>
  </bus>
  <bus id="bus26-11">
   <nodeMember connectorId="F25"/>
   <nodeMember connectorId="G25"/>
   <nodeMember connectorId="H25"/>
   <nodeMember connectorId="I25"/>
   <nodeMember connectorId="J25"/>
  </bus>
  <bus id="bus27-11">
   <nodeMember connectorId="F26"/>
   <nodeMember connectorId="G26"/>
   <nodeMember connectorId="H26"/>
   <nodeMember connectorId="I26"/>
   <nodeMember connectorId="J26"/>
  </bus>
  <bus id="bus28-11">
   <nodeMember connectorId="F27"/>
   <nodeMember connectorId="G27"/>
   <nodeMember connectorId="H27"/>
   <nodeMember connectorId="I27"/>
   <nodeMember connectorId="J27"/>
  </bus>
  <bus id="bus29-11">
   <nodeMember connectorId="F28"/>
   <nodeMember connectorId="G28"/>
   <nodeMember connectorId="H28"/>
   <nodeMember connectorId="I28"/>
   <nodeMember connectorId="J28"/>
  </bus>
  <bus id="bus30-11">
   <nodeMember connectorId="F29"/>
   <nodeMember connectorId="G29"/>
   <nodeMember connectorId="H29"/>
   <nodeMember connectorId="I29"/>
   <nodeMember connectorId="J29"/>
  </bus>
  <bus id="bus31-11">
   <nodeMember connectorId="F30"/>
   <nodeMember connectorId="G30"/>
   <nodeMember connectorId="H30"/>
   <nodeMember connectorId="I30"/>
   <nodeMember connectorId="J30"/>
  </bus>
  <bus id="bus32-11">
   <nodeMember connectorId="F31"/>
   <nodeMember connectorId="G31"/>
   <nodeMember connectorId="H31"/>
   <nodeMember connectorId="I31"/>
   <nodeMember connectorId="J31"/>
  </bus>
  <bus id="bus33-11">
   <nodeMember connectorId="F32"/>
   <nodeMember connectorId="G32"/>
   <nodeMember connectorId="H32"/>
   <nodeMember connectorId="I32"/>
   <nodeMember connectorId="J32"/>
  </bus>
  <bus id="bus34-11">
   <nodeMember connectorId="F33"/>
   <nodeMember connectorId="G33"/>
   <nodeMember connectorId="H33"/>
   <nodeMember connectorId="I33"/>
   <nodeMember connectorId="J33"/>
  </bus>
  <bus id="bus35-11">
   <nodeMember connectorId="F34"/>
   <nodeMember connectorId="G34"/>
   <nodeMember connectorId="H34"/>
   <nodeMember connectorId="I34"/>
   <nodeMember connectorId="J34"/>
  </bus>
  <bus id="bus36-11">
   <nodeMember connectorId="F35"/>
   <nodeMember connectorId="G35"/>
   <nodeMember connectorId="H35"/>
   <nodeMember connectorId="I35"/>
   <nodeMember connectorId="J35"/>
  </bus>
  <bus id="bus37-11">
   <nodeMember connectorId="F36"/>
   <nodeMember connectorId="G36"/>
   <nodeMember connectorId="H36"/>
   <nodeMember connectorId="I36"/>
   <nodeMember connectorId="J36"/>
  </bus>
  <bus id="bus38-11">
   <nodeMember connectorId="F37"/>
   <nodeMember connectorId="G37"/>
   <nodeMember connectorId="H37"/>
   <nodeMember connectorId="I37"/>
   <nodeMember connectorId="J37"/>
  </bus>
  <bus id="bus39-11">
   <nodeMember connectorId="F38"/>
   <nodeMember connectorId="G38"/>
   <nodeMember connectorId="H38"/>
   <nodeMember connectorId="I38"/>
   <nodeMember connectorId="J38"/>
  </bus>
  <bus id="bus40-11">
   <nodeMember connectorId="F39"/>
   <nodeMember connectorId="G39"/>
   <nodeMember connectorId="H39"/>
   <nodeMember connectorId="I39"/>
   <nodeMember connectorId="J39"/>
  </bus>
  <bus id="bus41-11">
   <nodeMember connectorId="F40"/>
   <nodeMember connectorId="G40"/>
   <nodeMember connectorId="H40"/>
   <nodeMember connectorId="I40"/>
   <nodeMember connectorId="J40"/>
  </bus>
  <bus id="bus42-11">
   <nodeMember connectorId="F41"/>
   <nodeMember connectorId="G41"/>
   <nodeMember connectorId="H41"/>
   <nodeMember connectorId="I41"/>
   <nodeMember connectorId="J41"/>
  </bus>
  <bus id="bus43-11">
   <nodeMember connectorId="F42"/>
   <nodeMember connectorId="G42"/>
   <nodeMember connectorId="H42"/>
   <nodeMember connectorId="I42"/>
   <nodeMember connectorId="J42"/>
  </bus>
  <bus id="bus44-11">
   <nodeMember connectorId="F43"/>
   <nodeMember connectorId="G43"/>
   <nodeMember connectorId="H43"/>
   <nodeMember connectorId="I43"/>
   <nodeMember connectorId="J43"/>
  </bus>
  <bus id="bus45-11">
   <nodeMember connectorId="F44"/>
   <nodeMember connectorId="G44"/>
   <nodeMember connectorId="H44"/>
   <nodeMember connectorId="I44"/>
   <nodeMember connectorId="J44"/>
  </bus>
  <bus id="bus46-11">
   <nodeMember connectorId="F45"/>
   <nodeMember connectorId="G45"/>
   <nodeMember connectorId="H45"/>
   <nodeMember connectorId="I45"/>
   <nodeMember connectorId="J45"/>
  </bus>
  <bus id="bus47-11">
   <nodeMember connectorId="F46"/>
   <nodeMember connectorId="G46"/>
   <nodeMember connectorId="H46"/>
   <nodeMember connectorId="I46"/>
   <nodeMember connectorId="J46"/>
  </bus>
  <bus id="bus48-11">
   <nodeMember connectorId="F47"/>
   <nodeMember connectorId="G47"/>
   <nodeMember connectorId="H47"/>
   <nodeMember connectorId="I47"/>
   <nodeMember connectorId="J47"/>
  </bus>
  <bus id="bus49-11">
   <nodeMember connectorId="F48"/>
   <nodeMember connectorId="G48"/>
   <nodeMember connectorId="H48"/>
   <nodeMember connectorId="I48"/>
   <nodeMember connectorId="J48"/>
  </bus>
  <bus id="bus50-11">
   <nodeMember connectorId="F49"/>
   <nodeMember connectorId="G49"/>
   <nodeMember connectorId="H49"/>
   <nodeMember connectorId="I49"/>
   <nodeMember connectorId="J49"/>
  </bus>
  <bus id="bus51-11">
   <nodeMember connectorId="F50"/>
   <nodeMember connectorId="G50"/>
   <nodeMember connectorId="H50"/>
   <nodeMember connectorId="I50"/>
   <nodeMember connectorId="J50"/>
  </bus>
  <bus id="bus52-11">
   <nodeMember connectorId="F51"/>
   <nodeMember connectorId="G51"/>
   <nodeMember connectorId="H51"/>
   <nodeMember connectorId="I51"/>
   <nodeMember connectorId="J51"/>
  </bus>
  <bus id="bus53-11">
   <nodeMember connectorId="F52"/>
   <nodeMember connectorId="G52"/>
   <nodeMember connectorId="H52"/>
   <nodeMember connectorId="I52"/>
   <nodeMember connectorId="J52"/>
  </bus>
  <bus id="bus54-11">
   <nodeMember connectorId="F53"/>
   <nodeMember connectorId="G53"/>
   <nodeMember connectorId="H53"/>
   <nodeMember connectorId="I53"/>
   <nodeMember connectorId="J53"/>
  </bus>
  <bus id="bus55-11">
   <nodeMember connectorId="F54"/>
   <nodeMember connectorId="G54"/>
   <nodeMember connectorId="H54"/>
   <nodeMember connectorId="I54"/>
   <nodeMember connectorId="J54"/>
  </bus>
  <bus id="bus56-11">
   <nodeMember connectorId="F55"/>
   <nodeMember connectorId="G55"/>
   <nodeMember connectorId="H55"/>
   <nodeMember connectorId="I55"/>
   <nodeMember connectorId="J55"/>
  </bus>
  <bus id="bus57-11">
   <nodeMember connectorId="F56"/>
   <nodeMember connectorId="G56"/>
   <nodeMember connectorId="H56"/>
   <nodeMember connectorId="I56"/>
   <nodeMember connectorId="J56"/>
  </bus>
  <bus id="bus58-11">
   <nodeMember connectorId="F57"/>
   <nodeMember connectorId="G57"/>
   <nodeMember connectorId="H57"/>
   <nodeMember connectorId="I57"/>
   <nodeMember connectorId="J57"/>
  </bus>
  <bus id="bus59-11">
   <nodeMember connectorId="F58"/>
   <nodeMember connectorId="G58"/>
   <nodeMember connectorId="H58"/>
   <nodeMember connectorId="I58"/>
   <nodeMember connectorId="J58"/>
  </bus>
  <bus id="bus60-11">
   <nodeMember connectorId="F59"/>
   <nodeMember connectorId="G59"/>
   <nodeMember connectorId="H59"/>
   <nodeMember connectorId="I59"/>
   <nodeMember connectorId="J59"/>
  </bus>
  <bus id="bus61-11">
   <nodeMember connectorId="F60"/>
   <nodeMember connectorId="G60"/>
   <nodeMember connectorId="H60"/>
   <nodeMember connectorId="I60"/>
   <nodeMember connectorId="J60"/>
  </bus>
  <bus id="bus62-11">
   <nodeMember connectorId="F61"/>
   <nodeMember connectorId="G61"/>
   <nodeMember connectorId="H61"/>
   <nodeMember connectorId="I61"/>
   <nodeMember connectorId="J61"/>
  </bus>
  <bus id="bus63-11">
   <nodeMember connectorId="F62"/>
   <nodeMember connectorId="G62"/>
   <nodeMember connectorId="H62"/>
   <nodeMember connectorId="I62"/>
   <nodeMember connectorId="J62"/>
  </bus>
  <bus id="busW-2">
   <nodeMember connectorId="W1"/>
   <nodeMember connectorId="W2"/>
   <nodeMember connectorId="W3"/>
   <nodeMember connectorId="W4"/>
   <nodeMember connectorId="W5"/>
   <nodeMember connectorId="W7"/>
   <nodeMember connectorId="W8"/>
   <nodeMember connectorId="W9"/>
   <nodeMember connectorId="W10"/>
   <nodeMember connectorId="W11"/>
   <nodeMember connectorId="W13"/>
   <nodeMember connectorId="W14"/>
   <nodeMember connectorId="W15"/>
   <nodeMember connectorId="W16"/>
   <nodeMember connectorId="W17"/>
   <nodeMember connectorId="W19"/>
   <nodeMember connectorId="W20"/>
   <nodeMember connectorId="W21"/>
   <nodeMember connectorId="W22"/>
   <nodeMember connectorId="W23"/>
   <nodeMember connectorId="W25"/>
   <nodeMember connectorId="W26"/>
   <nodeMember connectorId="W27"/>
   <nodeMember connectorId="W28"/>
   <nodeMember connectorId="W29"/>
  </bus>
  <bus id="busW-33">
   <nodeMember connectorId="W32"/>
   <nodeMember connectorId="W33"/>
   <nodeMember connectorId="W34"/>
   <nodeMember connectorId="W35"/>
   <nodeMember connectorId="W36"/>
   <nodeMember connectorId="W38"/>
   <nodeMember connectorId="W39"/>
   <nodeMember connectorId="W40"/>
   <nodeMember connectorId="W41"/>
   <nodeMember connectorId="W42"/>
   <nodeMember connectorId="W44"/>
   <nodeMember connectorId="W45"/>
   <nodeMember connectorId="W46"/>
   <nodeMember connectorId="W47"/>
   <nodeMember connectorId="W48"/>
   <nodeMember connectorId="W50"/>
   <nodeMember connectorId="W51"/>
   <nodeMember connectorId="W52"/>
   <nodeMember connectorId="W53"/>
   <nodeMember connectorId="W54"/>
   <nodeMember connectorId="W56"/>
   <nodeMember connectorId="W57"/>
   <nodeMember connectorId="W58"/>
   <nodeMember connectorId="W59"/>
   <nodeMember connectorId="W60"/>
  </bus>
  <bus id="busX-2">
   <nodeMember connectorId="X1"/>
   <nodeMember connectorId="X2"/>
   <nodeMember connectorId="X3"/>
   <nodeMember connectorId="X4"/>
   <nodeMember connectorId="X5"/>
   <nodeMember connectorId="X7"/>
   <nodeMember connectorId="X8"/>
   <nodeMember connectorId="X9"/>
   <nodeMember connectorId="X10"/>
   <nodeMember connectorId="X11"/>
   <nodeMember connectorId="X13"/>
   <nodeMember connectorId="X14"/>
   <nodeMember connectorId="X15"/>
   <nodeMember connectorId="X16"/>
   <nodeMember connectorId="X17"/>
   <nodeMember connectorId="X19"/>
   <nodeMember connectorId="X20"/>
   <nodeMember connectorId="X21"/>
   <nodeMember connectorId="X22"/>
   <nodeMember connectorId="X23"/>
   <nodeMember connectorId="X25"/>
   <nodeMember connectorId="X26"/>
   <nodeMember connectorId="X27"/>
   <nodeMember connectorId="X28"/>
   <nodeMember connectorId="X29"/>
  </bus>
  <bus id="busX-33">
   <nodeMember connectorId="X32"/>
   <nodeMember connectorId="X33"/>
   <nodeMember connectorId="X34"/>
   <nodeMember connectorId="X35"/>
   <nodeMember connectorId="X36"/>
   <nodeMember connectorId="X38"/>
   <nodeMember connectorId="X39"/>
   <nodeMember connectorId="X40"/>
   <nodeMember connectorId="X41"/>
   <nodeMember connectorId="X42"/>
   <nodeMember connectorId="X44"/>
   <nodeMember connectorId="X45"/>
   <nodeMember connectorId="X46"/>
   <nodeMember connectorId="X47"/>
   <nodeMember connectorId="X48"/>
   <nodeMember connectorId="X50"/>
   <nodeMember connectorId="X51"/>
   <nodeMember connectorId="X52"/>
   <nodeMember connectorId="X53"/>
   <nodeMember connectorId="X54"/>
   <nodeMember connectorId="X56"/>
   <nodeMember connectorId="X57"/>
   <nodeMember connectorId="X58"/>
   <nodeMember connectorId="X59"/>
   <nodeMember connectorId="X60"/>
  </bus>
  <bus id="busY-2">
   <nodeMember connectorId="Y1"/>
   <nodeMember connectorId="Y2"/>
   <nodeMember connectorId="Y3"/>
   <nodeMember connectorId="Y4"/>
   <nodeMember connectorId="Y5"/>
   <nodeMember connectorId="Y7"/>
   <nodeMember connectorId="Y8"/>
   <nodeMember connectorId="Y9"/>
   <nodeMember connectorId="Y10"/>
   <nodeMember connectorId="Y11"/>
   <nodeMember connectorId="Y13"/>
   <nodeMember connectorId="Y14"/>
   <nodeMember connectorId="Y15"/>
   <nodeMember connectorId="Y16"/>
   <nodeMember connectorId="Y17"/>
   <nodeMember connectorId="Y19"/>
   <nodeMember connectorId="Y20"/>
   <nodeMember connectorId="Y21"/>
   <nodeMember connectorId="Y22"/>
   <nodeMember connectorId="Y23"/>
   <nodeMember connectorId="Y25"/>
   <nodeMember connectorId="Y26"/>
   <nodeMember connectorId="Y27"/>
   <nodeMember connectorId="Y28"/>
   <nodeMember connectorId="Y29"/>
  </bus>
  <bus id="busY-33">
   <nodeMember connectorId="Y32"/>
   <nodeMember connectorId="Y33"/>
   <nodeMember connectorId="Y34"/>
   <nodeMember connectorId="Y35"/>
   <nodeMember connectorId="Y36"/>
   <nodeMember connectorId="Y38"/>
   <nodeMember connectorId="Y39"/>
   <nodeMember connectorId="Y40"/>
   <nodeMember connectorId="Y41"/>
   <nodeMember connectorId="Y42"/>
   <nodeMember connectorId="Y44"/>
   <nodeMember connectorId="Y45"/>
   <nodeMember connectorId="Y46"/>
   <nodeMember connectorId="Y47"/>
   <nodeMember connectorId="Y48"/>
   <nodeMember connectorId="Y50"/>
   <nodeMember connectorId="Y51"/>
   <nodeMember connectorId="Y52"/>
   <nodeMember connectorId="Y53"/>
   <nodeMember connectorId="Y54"/>
   <nodeMember connectorId="Y56"/>
   <nodeMember connectorId="Y57"/>
   <nodeMember connectorId="Y58"/>
   <nodeMember connectorId="Y59"/>
   <nodeMember connectorId="Y60"/>
  </bus>
  <bus id="busZ-2">
   <nodeMember connectorId="Z1"/>
   <nodeMember connectorId="Z2"/>
   <nodeMember connectorId="Z3"/>
   <nodeMember connectorId="Z4"/>
   <nodeMember connectorId="Z5"/>
   <nodeMember connectorId="Z7"/>
   <nodeMember connectorId="Z8"/>
   <nodeMember connectorId="Z9"/>
   <nodeMember connectorId="Z10"/>
   <nodeMember connectorId="Z11"/>
   <nodeMember connectorId="Z13"/>
   <nodeMember connectorId="Z14"/>
   <nodeMember connectorId="Z15"/>
   <nodeMember connectorId="Z16"/>
   <nodeMember connectorId="Z17"/>
   <nodeMember connectorId="Z19"/>
   <nodeMember connectorId="Z20"/>
   <nodeMember connectorId="Z21"/>
   <nodeMember connectorId="Z22"/>
   <nodeMember connectorId="Z23"/>
   <nodeMember connectorId="Z25"/>
   <nodeMember connectorId="Z26"/>
   <nodeMember connectorId="Z27"/>
   <nodeMember connectorId="Z28"/>
   <nodeMember connectorId="Z29"/>
  </bus>
  <bus id="busZ-33">
   <nodeMember connectorId="Z32"/>
   <nodeMember connectorId="Z33"/>
   <nodeMember connectorId="Z34"/>
   <nodeMember connectorId="Z35"/>
   <nodeMember connectorId="Z36"/>
   <nodeMember connectorId="Z38"/>
   <nodeMember connectorId="Z39"/>
   <nodeMember connectorId="Z40"/>
   <nodeMember connectorId="Z41"/>
   <nodeMember connectorId="Z42"/>
   <nodeMember connectorId="Z44"/>
   <nodeMember connectorId="Z45"/>
   <nodeMember connectorId="Z46"/>
   <nodeMember connectorId="Z47"/>
   <nodeMember connectorId="Z48"/>
   <nodeMember connectorId="Z50"/>
   <nodeMember connectorId="Z51"/>
   <nodeMember connectorId="Z52"/>
   <nodeMember connectorId="Z53"/>
   <nodeMember connectorId="Z54"/>
   <nodeMember connectorId="Z56"/>
   <nodeMember connectorId="Z57"/>
   <nodeMember connectorId="Z58"/>
   <nodeMember connectorId="Z59"/>
   <nodeMember connectorId="Z60"/>
  </bus>
 </buses>
</module>