<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='trimmer_smd1VariableCapacitorModuleID'>
<version>4</version>
<date>2012-02-03</date>
<author>jonathan</author>
<description></description>
<title>Variable Capacitor</title>
<tags>
<tag>capacitor</tag>
<tag>variable</tag>
</tags>
<properties>
<property name='max capacitance'>10pF</property>
<property name='family'>variable capacitor</property>
<property name='type'>4x6mm, outer Pads</property>
<property name='min capacitance'>2pF</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/capacitor_variable_2_legs.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/capacitor_variable_2_legs.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/trimmer_smd1_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/capacitor_variable_2_legs.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='male' name='0'>
<description>0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='male' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
